DICOM PS3.3 2021c - Information Object Definitions

A.8.3.5 Multi-frame Grayscale Byte SC Image Functional Group Macros (Current)
Prev | A.8.3 Multi-frame Grayscale Byte Secondary Capture Image IOD | Next

#### A.8.3.5 Multi-frame Grayscale Byte SC Image Functional Group Macros

Table A.8-3b specifies the use of the Functional Group Macros used in the Multi-frame Functional Groups Module for the Multi-frame Grayscale Byte SC Image IOD.

Table A.8-3b. Multi-frame Grayscale Byte SC Image Functional Group Macros

Functional Group Macro | Section | Usage
--- | --- | ---
Pixel Measures | C.7.6.16.2.1 | C - Required if Plane Position (Patient) or Plane Orientation (Patient) Macros Present
Plane Position (Patient) | C.7.6.16.2.3 | C - Required if Pixel Measures or Plane Orientation (Patient) Macros Present
Plane Orientation (Patient) | C.7.6.16.2.4 | C - Required if Pixel Measures or Plane Position (Patient) Macros Present

Prev | Up | Next
A.8.3.4 Multi-frame Grayscale Byte SC Image IOD Content Constraints | Home | A.8.4 Multi-frame Grayscale Word Secondary Capture Image IOD

DICOM PS3.3 2021c - Information Object Definitions