DICOM PS3.17 2021c - Explanatory Information

TTTT.2 Frame of Reference (Current)
Prev | TTTT Dermoscopy (Informative) | Next

## TTTT.2 Frame of Reference

Some dermoscopes record multiple images during a single acquisition with each acquisition using a different lighting mode. The dermoscope does not move during acquisition therefore the corresponding pixel in each image is of exactly the same region of skin. In this scenario a vendor generated unique identifier can be encoded in the (0020,0052) Frame of Reference UID attribute for all images acquired during the acquisition.

Prev | Up | Next
TTTT Dermoscopy (Informative) | Home | TTTT.3 Use Cases

DICOM PS3.17 2021c - Explanatory Information