DICOM PS3.3 2021c - Information Object Definitions

C.7.6.28 Real-Time Acquisition Module (Current)
Prev | C.7.6 Common Image IE Modules | Next

#### C.7.6.28 Real-Time Acquisition Module

Table C.7.6.28-1 defines the Attributes related to all frames when the IOD is transported using Real-Time Communication.

Table C.7.6.28-1. Real-Time Acquisition Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Shared Functional Group Sequence | (5200,9229) | 1 | Sequence that contains the Functional Group Macros that are shared for all frames. Only a single Item shall be included in this Sequence.
>Include one or more Functional Group Macros that are shared by all frames. | For each IOD that includes this module, a table is defined in which the permitted Functional Group Macros and their usage is specified. The Item may be empty if the requirements for inclusion of the Functional Groups are not satisfied.
Stereo Pairs Present | (0022,0028) | 1 | The multi-frame pixel data consists of left and right stereoscopic pairs. See Section C.7.6.28.1.1 for further explanation. Enumerated Values: YES NO

##### C.7.6.28.1 Real-Time Acquisition Module Attributes

###### C.7.6.28.1.1 Stereo Pairs Present

Stereo Pairs Present (0022,0028) shall have the value of YES when frame is encoded as left and right stereoscopic pair.

Prev | Up | Next
C.7.6.27 Current Frame Functional Groups Module | Home | C.7.7 Patient Summary Module

DICOM PS3.3 2021c - Information Object Definitions