DICOM PS3.16 2021c - Content Mapping Resource

CID 6311 MR Signal Intensity (Current)
Prev | B DCMR Context Groups (Normative) | Next

## CID 6311 MR Signal Intensity

This context group contains terms specific to describing the types of MR sequences used in mpMRI of the prostate.

### Note

Imaging findings will be applicable for indications other than PI-RADS® disease assessment.

Resources:

  HTML | FHIR JSON | FHIR XML | IHE SVS XML

Type:

  Extensible

Version:

  20210714

UID:

  1.2.840.10008.6.1.1368

Table CID 6311. MR Signal Intensity

Coding Scheme Designator | Code Value | Code Meaning | SNOMED-RT ID | UMLS Concept Unique ID
--- | --- | --- | --- | ---
DCM | 110805 | T2 Weighted MR Signal Intensity |  |
DCM | 113043 | Diffusion weighted |  |
DCM | 130566 | Diffusion-weighted Acquisition Highest b-value image |  |
DCM | 130567 | Dynamic Contrast-Enhanced Acquisition |  |
DCM | 130568 | Dynamic Contrast-Enhanced Acquisition Subtraction image |  |
DCM | 110804 | T1 Weighted MR Signal Intensity |  |
DCM | 113041 | Apparent Diffusion Coefficient |  |

Prev | Up | Next
CID 6310 Prostate Reporting Systems | Home | CID 6312 Cross-sectional Scan Plane Orientation

DICOM PS3.16 2021c - Content Mapping Resource