DICOM PS3.5 2021d - Data Structures and Encoding

10.17 Transfer Syntax for SMPTE ST 2110-30 PCM Digital Audio (Current)
Prev | 10 Transfer Syntax | Next

## 10.17 Transfer Syntax for SMPTE ST 2110-30 PCM Digital Audio

This Transfer Syntax is used for audio channel data carried in a DICOM-RTV Flow (separated from DICOM-RTV Metadata Flow) as described by [SMPTE ST 2110-30]. The main parameters of the transfer syntax are described in Section A.10.

Prev | Up | Next
10.16 Transfer Syntax for SMPTE ST 2110-20 Uncompressed Interlaced Active Video | Home | A Transfer Syntax Specifications (Normative)

DICOM PS3.5 2021d - Data Structures and Encoding