DICOM PS3.4 2021d - Service Class Specifications

J.3.6.2 SCP Conformance. (Current)
Prev | J.3.6 Conformance Requirements | Next

#### J.3.6.2 SCP Conformance.

An implementation that is conformant to this SOP Class as an SCP shall meet conformance requirements for

- the operations and actions that it performs

- the notifications that it generates.

##### J.3.6.2.1 Operations

The SCP shall document in the SCP Operations Statement the behavior and actions of the SCP upon receiving the N-ACTION primitive (Storage Commitment Request).

The SCP shall specify parameters indicating the level of storage commitment, such as:

- under what conditions the SCP would delete SOP Instances

- persistence of storage

- capacity

- volatility

- other pertinent information

The SCP shall specify the mechanisms and characteristics of retrieval of stored SOP Instances, such as:

- supported query/retrieve services

- latency

- other pertinent information

The SCP shall specify if it supports the optional Storage Media File-Set ID & UID Attributes in the N-ACTION. If these Attributes are supported, the SCP shall also specify which Storage Media Application Profiles are supported.

The SCP Operations Statement shall be formatted as defined in PS3.2

Prev | Up | Next
J.3.6 Conformance Requirements | Home | J.3.6.2.2 Notifications

DICOM PS3.4 2021d - Service Class Specifications