DICOM PS3.3 2021d - Information Object Definitions

C.7.6.14 Acquisition Context Module (Current)
Prev | C.7.6 Common Image IE Modules | Next

#### C.7.6.14 Acquisition Context Module

Table C.7.6.14-1 specifies Attributes for description of the conditions present during data acquisition.

This Module shall not contain descriptions of conditions that replace those that are already described in specific Modules or Attributes that are also contained within the IOD that contains this Module.

### Note

1. If this SOP Instance is a Multi-frame SOP Instance, each Item of the Acquisition Context Sequence (0040,0555) may be configured to describe one frame, all frames, or any specifically enumerated subset set of frames of the Multi-frame SOP Instance. Previously, Referenced Frame Numbers (0040,A136) was used to enumerate which frames were described, but its length was limited, so it has been replaced by Referenced Frame Number (0008,1160). Similarly, applicability to a subset of Segments or Waveform Channels may be specified.

Table C.7.6.14-1. Acquisition Context Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Acquisition Context Sequence | (0040,0555) | 2 | A Sequence of Items that describes the conditions present during the acquisition of the data of the SOP Instance. Zero or more Items shall be included in this Sequence.
>Include Table 10.2.1-1 “Content Item with Modifiers Macro Attributes”
Acquisition Context Description | (0040,0556) | 3 | Free-text description of the image-acquisition context.

Prev | Up | Next
C.7.6.13 Intervention Module | Home | C.7.6.15 Bitmap Display Shutter Module

DICOM PS3.3 2021d - Information Object Definitions