DICOM PS3.16 2021d - Content Mapping Resource

TID 10054 Procedure Characteristics (Current)
Prev | Enhanced X-Ray Radiation Dose SR IOD Templates | Next

### TID 10054 Procedure Characteristics

This template describes the details of the procedure characteristics (e.g., patient orientation, SID, etc.).

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 10054. Procedure Characteristics

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (130530, DCM, "Procedure Characteristics") | 1 | M |  |
2 | > | CONTAINS | DATETIME | DT (111526, DCM, "DateTime Started") | 1 | M |  |
3 | > | CONTAINS | DATETIME | DT (111527, DCM, "DateTime Ended") | 1 | M |  |
4 | > | CONTAINS | NUM | EV (113832, DCM, "Identification of the X-Ray Source") | 1 | M |  | UNITS = EV (1, UCUM, "no units")
5 | > | CONTAINS | TEXT | EV (125203, DCM, "Acquisition Protocol") | 1 | U |  |
6 | > | CONTAINS | CODE | EV (113745, DCM, "Patient Table Relationship") | 1 | U |  | DCID 21 “Patient Equipment Relationship”
7 | > | CONTAINS | CODE | EV (113743, DCM, "Patient Orientation") | 1 | U |  | DCID 19 “Patient Orientation”
8 | >> | HAS CONCEPT MOD | CODE | EV (113744, DCM, "Patient Orientation Modifier") | 1 | M |  | DCID 20 “Patient Orientation Modifier”
9 | > | CONTAINS | CODE | EV (123014, DCM, "Target Region") | 1 | U |  | DCID 4016 “Anatomic Region for Intra-oral Radiography” DCID 4026 “Primary Anatomic Structure for Intra-oral and Craniofacial Radiography - Teeth” DCID 4028 “Craniofacial Anatomic Regions” DCID 4030 “CT, MR and PET Anatomy Imaged” DCID 4031 “Common Anatomic Regions”
10 | >> | HAS CONCEPT MOD | CODE | EV (272741003, SCT, "Laterality") | 1 | UC | IF target region is bilateral | DCID 244 “Laterality”
11 | > | CONTAINS | CODE | EV (111635, DCM, "X-Ray Grid") | 1-n | U |  | DCID 10017 “X-Ray Grid”
12 | > | CONTAINS | NUM | EV (113750, DCM, "Distance Source to Detector") | 1 | UC | XOR Row 13 | UNITS = EV (mm, UCUM, "mm")
13 | > | CONTAINS | TABLE | EV (113750, DCM, "Distance Source to Detector") | 1 | UC | XOR Row 12 | NCOLUMNS = 2 COLUMN 1 = EV (111526, DCM, "DateTime Started") EV (113750, DCM, "Distance Source to Detector") COLUMN 2 UNITS = EV (mm, UCUM, "mm") COLUMN 1 VR = DT COLUMN 2 VR = FL

Content Item Descriptions

Row 2 | The DateTime of the beginning of the time period over which the content items are applicable.
Row 3 | The DateTime of the end of the time period over which the content items are applicable.
Row 4 | Identification the X-Ray source. This designation shall not change for a given source throughout the entire RDSR. For systems with multiple X-Ray sources, each source shall be described with a separate instance of this template.

Prev | Up | Next
TID 10053 Patient Attenuation Characteristics | Home | TID 10055 Attenuator Characteristics

DICOM PS3.16 2021d - Content Mapping Resource