DICOM PS3.4 2021d - Service Class Specifications

DD.3.2.2.2 Attributes (Current)
Prev | DD.3.2.2 N-GET | Next

##### DD.3.2.2.2 Attributes

The Attribute list of the N-GET for the RT Conventional Machine Verification SOP Class and RT Ion Machine Verification SOP Class is shown in Table DD.3.2.2.2-1. See Section 5.4 for usage notation.

Table DD.3.2.2.2-1. N-GET Attribute List- RT Conventional Machine Verification SOP Class and RT Ion Machine Verification SOP Class

Attribute Name | Tag | Usage SCU/SCP
--- | --- | ---
Referenced RT Plan Sequence | (300C,0002) | -/1
>Referenced SOP Class UID | (0008,1150) | -/1
>Referenced SOP Instance UID | (0008,1155) | -/1
Referenced Fraction Group Number | (300C,0022) | -/1
Patient ID | (0010,0020) | -/1
Include Table CC.2.5-2e “Issuer of Patient ID Macro”
Treatment Verification Status | (3008,002C) | -/1
Failed Parameters Sequence | (0074,1048) | -/2 (zero or more items shall be included in this Sequence)
>Include Table DD.3.2.2.1-1 “Verification Parameters Selector Attribute Macro”
Overridden Parameters Sequence | (0074,104A) | -/2 (zero or more items shall be included in this Sequence)
>Include Table DD.3.2.2.1-1 “Verification Parameters Selector Attribute Macro”
>Operators' Name | (0008,1070) | -/2
>Override Reason | (3008,0066) | -/2
All other Attributes | - | 3/2

Prev | Up | Next
DD.3.2.2 N-GET | Home | DD.3.2.2.3 Status

DICOM PS3.4 2021d - Service Class Specifications