DICOM PS3.3 2021d - Information Object Definitions

A.34.16.4.5 Waveform Sample Interpretation (Current)
Prev | A.34.16.4 Multi-channel Respiratory Waveform IOD Constraints | Next

##### A.34.16.4.5 Waveform Sample Interpretation

The value of Waveform Sample Interpretation (5400,1006) in each Waveform Sequence Item shall be SS or SL.

Prev | Up | Next
A.34.16.4.4 Channel Source and Channel Source Modifiers | Home | A.34.16.4.6 Waveform Annotation Module

DICOM PS3.3 2021d - Information Object Definitions