DICOM PS3.16 2021d - Content Mapping Resource

CID 6 Transducer Orientation (Current)
Prev | B DCMR Context Groups (Normative) | Next

## CID 6 Transducer Orientation

Resources:

  HTML | FHIR JSON | FHIR XML | IHE SVS XML

Type:

  Extensible

Version:

  20190817

UID:

  1.2.840.10008.6.1.4

Table CID 6. Transducer Orientation

Coding Scheme Designator | Code Value | Code Meaning | SNOMED-RT ID | UMLS Concept Unique ID
--- | --- | --- | --- | ---
SCT | 81654009 | Coronal | G-A138 | C0205123
SCT | 38717003 | Longitudinal | G-A143 | C0205127
SCT | 30730003 | Sagittal | G-A145 | C0205129
SCT | 103343002 | Parasagittal | G-A189 | C0522491
SCT | 21114003 | Oblique | G-A472 | C0205315
SCT | 103339001 | Long axis | G-A185 | C0522487
SCT | 103341000 | Off axis | G-A187 | C0522489
SCT | 103340004 | Short axis | G-A186 | C0522488
SCT | 398994001 | Five chamber | G-A191 | C1302157
SCT | 399232001 | Two chamber | G-A19B | C1302267
SCT | 399214001 | Four chamber | G-A19C | C1302256
SCT | 62824007 | Transverse | G-A117 | C0205106

### Note

1. In a prior version of this table, the code G-A11B was specified for the concept Parasagittal. The use of this code conflicts with its assignment to another concept in SNOMED, and its use in this context is deprecated. Although there is minimal possibility of misinterpretation with SOP Instances that may include the deprecated use, receiving applications should be aware of this change; see Annex J.

2. In a prior version of this table, the code G-A13B was specified for the concept of "Off axis", whereas that code actually means "Unilateral left (qualifier value)".

Prev | Up | Next
CID 5 Transducer Approach | Home | CID 7 Ultrasound Beam Path

DICOM PS3.16 2021d - Content Mapping Resource