DICOM PS3.8 2021d - Network Communication Support for Message Exchange

7.3 A-ABORT Service (Current)
Prev | 7 OSI Upper Layer Service for DICOM Application Entities | Next

## 7.3 A-ABORT Service

The ACSE A-ABORT service shall be used by a requestor in either of the AEs to cause the abnormal release of the association. It shall be a non-confirmed service. However, because of the possibility of an A-ABORT service procedure collision, the delivery of the indication primitive is not guaranteed. Should such a collision occur, both AEs are aware that the association has been terminated. The abort shall be performed through A-ABORT request and A-ABORT indication primitives.

### Note

An A-ABORT request primitive used on an established association may result in the destruction of data in transit.

Figure 7-3 illustrates aborting an established association between two AE's.

Figure 7-3. Association User Initiated Abort

### 7.3.1 A-ABORT Parameters

Table 7-5 lists the parameters for the A-ABORT service. Only the first parameter shall be used by DICOM Application Entities in this Standard.

Table 7-5. A-ABORT Service Parameters

A-ABORT Parameter Name | Request | Indication
--- | --- | ---
abort source |  | M
user information | NU | NU(=)

#### 7.3.1.1 Abort Source

This parameter indicates the initiating source of this abort. It shall take one of the following symbolic values:

1. UL service-user

2. UL service-provider (ACSE related)

Prev | Up | Next
7.2.2 A-RELEASE Service Procedure | Home | 7.3.2 A-ABORT Service Procedure

DICOM PS3.8 2021d - Network Communication Support for Message Exchange