DICOM PS3.3 2021d - Information Object Definitions

C.36.13 RT Radiation Common Module (Current)
Prev | C.36 RT Second Generation Modules | Next

### C.36.13 RT Radiation Common Module

The RT Radiation Common Module contains the Attributes shared by all RT Radiation IODs used for radiation treatment delivery.

Table C.36.13-1. RT Radiation Common Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Include Table 10.9.1-1 “Enhanced Content Identification Macro Attributes”.
Include Table C.36.2.1.6-1 “RT Radiation Common Base Macro Attributes”.
Treatment Time Limit | (300A,062E) | 3 | The maximum delivery time in seconds. See Section C.36.13.1.3.

#### C.36.13.1 RT Radiation Common Attribute Descriptions

##### C.36.13.1.1 Radiotherapy Procedure Technique Sequence

See Section C.36.2.1.6.1.1.

##### C.36.13.1.2 RT Treatment Position Macro

See Section C.36.2.1.6.1.2.

##### C.36.13.1.3 Treatment Time Limit

The Treatment Time Limit (300A,062E) is the maximum time span allowed to deliver a single fraction of this RT Radiation SOP Instance. The behavior of the treatment delivery device on exceeding the Treatment Time Limit is up to the implementation. Treatment is expected to terminate upon reaching the Treatment Time Limit (300A,062E) independent of the Meterset and so this Attribute should have a value that accommodates normal variations in delivery.

##### C.36.13.1.4 Treatment Machine Special Mode Sequence

See Section C.36.2.1.6.1.3.

Prev | Up | Next
C.36.12.2.2 Standard Robotic-Arm Coordinate System Frame of Reference | Home | C.36.14 C-Arm Photon-Electron Delivery Device Module

DICOM PS3.3 2021d - Information Object Definitions