DICOM PS3.3 2021d - Information Object Definitions

A.34.11.4.4 Sampling Frequency (Current)
Prev | A.34.11.4 Real-Time Audio Waveform IOD Content Constraints | Next

##### A.34.11.4.4 Sampling Frequency

The value of Sampling Frequency (003A,001A) in each Waveform Sequence Item shall be 44.1 kHz, 48 kHz, or 96 kHz.

Prev | Up | Next
A.34.11.4.3 Number of Waveform Channels | Home | A.34.11.4.5 Channel Source

DICOM PS3.3 2021d - Information Object Definitions