DICOM PS3.2 2021d - Conformance

E.8.5.3 Standard Extended Basic Grayscale Image Box SOP Class (Current)
Prev | E.8.5 Standard Extended / Specialized / Private SOP Classes | Next

#### E.8.5.3 Standard Extended Basic Grayscale Image Box SOP Class

SOP Class : Basic Grayscale Image Box SOP

Attribute : Bits Stored (0028,0028)

Extensions : 8-16 bits stored are supported.

DICOM only specifies 8 and 12 for number of bits stored. The EXAMPLE-PRINT-SERVER-MANAGEMENT supports the number of bits stored to be from 8 through 16 bits.

SOP Class : Basic Grayscale Image Box SOP

Attribute : High Bit (0028,0028)

Extensions : High Bit positions 7 - 15 are supported.

DICOM specifies that the high bit must be the 7th or 11th bit (for 8 or 12 bits stored, respectively). The EXAMPLE-PRINT-SERVER-MANAGEMENT supports the high bit to be the number of bits stored minus one. For example, if the number of bits stored is 13, the high bit is 12.

Prev | Up | Next
E.8.5.2 Standard Extended Basic Film Box SOP Class | Home | E.8.6 Private Transfer Syntaxes

DICOM PS3.2 2021d - Conformance