DICOM PS3.3 2021d - Information Object Definitions

A.35.5.3 Mammography CAD SR IOD Module Table (Current)
Prev | A.35.5 Mammography CAD SR IOD | Next

#### A.35.5.3 Mammography CAD SR IOD Module Table

Table A.35.5-1 specifies the Modules of the Mammography CAD SR IOD.

Table A.35.5-1. Mammography CAD SR IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | SR Document Series | C.17.1 | M
Clinical Trial Series | C.7.3.2 | U
Equipment | General Equipment | C.7.5.1 | M
Document | SR Document General | C.17.2 | M
SR Document Content | C.17.3 | M
SOP Common | C.12.1 | M

### Note

The Specimen Identification Module was previously included in this IOD but has been retired. See PS3.3-2008.

##### A.35.5.3.1 Mammography CAD SR IOD Content Constraints

###### A.35.5.3.1.1 Template Constraints

The document shall be constructed from TID 4000 “Mammography CAD Document Root” invoked at the root node.

When a Content Item sub-tree from a prior document is duplicated by-value, its observation context shall be defined by TID 1001 “Observation Context” and its subordinate templates.

### Note

All Template and Context Group definitions are located in Annex A “Structured Reporting Templates (Normative)” in PS3.16 and Annex B “DCMR Context Groups (Normative)” in PS3.16, respectively.

###### A.35.5.3.1.2 Value Type

Value Type (0040,A040) in Content Sequence (0040,A730) of the SR Document Content Module is constrained to the following Enumerated Values (see Table C.17.3-7 for Value Type definitions):

Enumerated Values:

TEXT

CODE

NUM

DATE

TIME

UIDREF

PNAME

SCOORD

COMPOSITE

IMAGE

CONTAINER

###### A.35.5.3.1.3 Relationship Constraints

The Mammography CAD SR IOD makes extensive use of by-reference INFERRED FROM, by-reference HAS PROPERTIES and by-reference SELECTED FROM relationships. Other relationships by-reference are forbidden. Table A.35.5-2 specifies the relationship constraints of this IOD. See Table C.17.3-8 for Relationship Type definitions.

Table A.35.5-2. Relationship Content Constraints for Mammography CAD SR IOD

Source Value Type | Relationship Type (Enumerated Values) | Target Value Type
--- | --- | ---
CONTAINER | CONTAINS | CODE, NUM, SCOORD, IMAGE1, CONTAINER, TEXT, DATE
TEXT, CODE, NUM, CONTAINER | HAS OBS CONTEXT | TEXT, CODE, NUM, DATE, TIME, PNAME, UIDREF, COMPOSITE1
CONTAINER | HAS OBS CONTEXT | CONTAINER
IMAGE | HAS ACQ CONTEXT | TEXT, CODE, DATE, TIME, NUM, UIDREF
CONTAINER, CODE, NUM, COMPOSITE | HAS CONCEPT MOD | TEXT, CODE2.
TEXT, CODE, NUM | HAS PROPERTIES | CONTAINER, TEXT, CODE, NUM, DATE, IMAGE1, SCOORD, UIDREF
CODE, NUM | INFERRED FROM | CODE, NUM, SCOORD, CONTAINER, TEXT, IMAGE
SCOORD | SELECTED FROM | IMAGE1

### Note

1. Which SOP Classes the IMAGE or COMPOSITE Value Type may refer to, is documented in the Conformance Statement for an application (see PS3.2 and PS3.4).

2. The HAS CONCEPT MOD relationship is used to modify the meaning of the Concept Name of a Source Content Item, for example to provide a more descriptive explanation, a different language translation, or to define a post-coordinated concept.

Prev | Up | Next
A.35.5.2 Mammography CAD SR IOD Entity-Relationship Model | Home | A.35.6 Chest CAD SR IOD

DICOM PS3.3 2021d - Information Object Definitions