DICOM PS3.3 2021d - Information Object Definitions

C.8.8.14.16 Referenced Control Point (Current)
Prev | C.8.8.14 RT Beams Module | Next

##### C.8.8.14.16 Referenced Control Point

The number of Items in the Beam Dose Verification Control Point Sequence (300A,008C) is not required to be the same as in the Control Point Sequence (300A,0111). A different sampling can be chosen for the Beam Dose Verification Control Point Sequence, but where the Cumulative Meterset Weight of a Control Point Sequence (300A,008C) Item is the same it shall be referenced by the Referenced Control Point Index (300C,00F0).

Prev | Up | Next
C.8.8.14.15 Source to External Contour Distance and External Contour Entry Point | Home | C.8.8.15 RT Brachy Application Setups Module

DICOM PS3.3 2021d - Information Object Definitions