DICOM PS3.3 2021d - Information Object Definitions

A.34.2.4.5 Waveform Sample Interpretation (Current)
Prev | A.34.2.4 Basic Voice Audio IOD Content Constraints | Next

##### A.34.2.4.5 Waveform Sample Interpretation

The value of Waveform Sample Interpretation (5400,1006) in the Waveform Sequence (5400,0100) Item shall be UB, MB, or AB.

Prev | Up | Next
A.34.2.4.4 Sampling Frequency | Home | A.34.3 12-Lead ECG IOD

DICOM PS3.3 2021d - Information Object Definitions