DICOM PS3.16 2021d - Content Mapping Resource

CID 9575 Patient Alignment Devices (Current)
Prev | B DCMR Context Groups (Normative) | Next

## CID 9575 Patient Alignment Devices

Resources:

  HTML | FHIR JSON | FHIR XML | IHE SVS XML

Type:

  Extensible

Version:

  20210906

UID:

  1.2.840.10008.6.1.1422

Table CID 9575. Patient Alignment Devices

Coding Scheme Designator | Code Value | Code Meaning | SNOMED-RT ID | UMLS Concept Unique ID
--- | --- | --- | --- | ---
DCM | 128151 | Laser Cross-hairs |  |
DCM | 130642 | Optical Distance Meter |  |
DCM | 130643 | Mechanical Pointer |  |
DCM | 130644 | Radiofrequency Transponder |  |
DCM | OSS | Optical Surface Scanner |  |
DCM | LS | Laser Surface Scan |  |
DCM | 130645 | Infrared Marker |  |
DCM | 130646 | Radioactive Marker |  |
DCM | 130647 | Thermal Imager |  |
DCM | 130648 | Combined Structured Light/Thermal Imager |  |
DCM | 130649 | Ocular Fixation Light |  |

Prev | Up | Next
CID 9574 Patient Position Displacement Reference Points | Home | CID 9576 Reasons for RT Radiation Treatment Omission

DICOM PS3.16 2021d - Content Mapping Resource