DICOM PS3.17 2021d - Explanatory Information

XXX.4 Uses of Presentation View Description in the Identification Module (Current)
Prev | XXX Volumetric Presentation States (Informative) | Next

## XXX.4 Uses of Presentation View Description in the Identification Module

### XXX.4.1 Hanging Protocols

A Hanging Protocol Instance could select a set of orthogonal MPRs by use of the Image Sets Sequence (0072,0020).

Table XXX.4.1-1. Hanging Protocol Image Set Sequence Recommendations

Attribute Name | Tag | Comment
--- | --- | ---
Image Sets Sequence | (0072,0020) |
>Image Set Selector Sequence | (0072,0022) |
>>Image Set Selector Usage Flag | (0072,0024) | Set to "MATCH"
>>Selector Attribute | (0072,0026) | Set to "0008,0016", the SOP Class UID Attribute Tag
>>Selector Attribute VR | (0072,0050) | Set to "UI", the SOP Class UID Attribute VR
>>Selector UI Value[i] | (0072,XXXX) | Set to "1.2.840.10008.​5.​1.​4.​1.​1.​11.​6", SOP Class UID of the Planar MPR VPS SOP Class
>>Image Set Selector Usage Flag | (0072,0024) | Set to "MATCH"
>>Selector Attribute | (0072,0026) | Set to "0054,0220", the View Code Sequence Attribute Tag
>>Selector Attribute VR | (0072,0050) | Set to "SQ", the View Code Sequence Attribute VR
>>Selector Code Value | (0072,0080) | Set to (81654009, SCT, "Coronal")
>>Image Set Number | (0072,0032) | Set to "1" for Image Set 1
>>Image Set Selector Usage Flag | (0072,0024) | Set to "MATCH"
>>Selector Attribute | (0072,0026) | Set to "0008,0016", the SOP Class UID Attribute Tag
>>Selector Attribute VR | (0072,0050) | Set to "UI", the SOP Class UID Attribute VR
>>Selector UI Value | (0072,XXXX) | Set to "1.2.840.10008.​5.​1.​4.​1.​1.​11.​6", SOP Class UID of the Planar MPR VPS SOP Class
>>Image Set Selector Usage Flag | (0072,0024) | Set to "MATCH"
>>Selector Attribute | (0072,0026) | Set to "0054,0220", the View Code Sequence Attribute Tag
>>Selector Attribute VR | (0072,0050) | Set to "SQ", the View Code Sequence Attribute VR
>>Selector Code Value | (0072,0080) | Set to (30730003, SCT, "Sagittal")
>>Image Set Number | (0072,0032) | Set to "2" for Image Set 2
>>Image Set Selector Usage Flag | (0072,0024) | Set to "MATCH"
>>Selector Attribute | (0072,0026) | Set to "0008,0016", the SOP Class UID Attribute Tag
>>Selector Attribute VR | (0072,0050) | Set to "UI", the SOP Class UID Attribute VR
>>Selector UI Value | (0072,XXXX) | Set to "1.2.840.10008.​5.​1.​4.​1.​1.​11.​6", SOP Class UID of the Planar MPR VPS SOP Class
>>Image Set Selector Usage Flag | (0072,0024) | Set to "MATCH"
>>Selector Attribute | (0072,0026) | Set to "0054,0220", the View Code Sequence Attribute Tag
>>Selector Attribute VR | (0072,0050) | Set to "SQ", the View Code Sequence Attribute VR
>>Selector Code Value | (0072,0080) | Set to (62824007, SCT, "Transverse")
>>Image Set Number | (0072,0032) | Set to "3" for Image Set 3

The display application would look for three Planar MPR Volumetric Presentation States - one Coronal, one Sagittal and one Transverse - and associate them with Image Sets in the view.

Prev | Up | Next
XXX.3.12.3.5 Render Display Module Recommendations | Home | XXX.4.2 Structured Displays

DICOM PS3.17 2021d - Explanatory Information