DICOM PS3.2 2021d - Conformance

L.4.2 AE Specifications (Current)
Prev | L.4 Networking | Next

### L.4.2 AE Specifications

This AE complies with Section 6.2 “Transport” in PS3.22 , specification for DICOM-RTV.

#### L.4.2.1 DICOM-RTV Application Entity Specifications

##### L.4.2.1.1 SOP Classes

EXAMPLE-RTV-SERVICE provides Standard Conformance to the following SOP Classes:

Table L.4.2-1. SOP Classes for DICOM-RTV AE

SOP Class Name | SOP Class UID | SCU | SCP
--- | --- | --- | ---
Video Photographic Image Real-Time Communication | 1.2.840.10008.10.2 | No | Yes

Some restrictions applies on the Real-Time Communications:

Table L.4.2-2. DICOM-RTV Instances Specification

Category | Restrictions
--- | ---
Transfer Syntaxes Supported | SMPTE ST 2110-20 Uncompressed Progressive Active Video
Photometric interpretation | RGB
Bit depth | 10

Table L.4.2-3. DICOM-RTV Screen Resolutions

Rows | Columns | Frame rate | Video Type | Progressive or Interlaced
--- | --- | --- | --- | ---
1080 | 1920 | 25 | 25 Hz HD | P
1080 | 1920 | 29.97, 30 | 30 Hz HD | P
1080 | 1920 | 25 | 25 Hz HD | I
1080 | 1920 | 29.97, 30 | 30 Hz HD | I
720 | 1280 | 25 | 25 Hz HD | P
720 | 1280 | 29.97, 30 | 30 Hz HD | P
720 | 1280 | 50 | 50 Hz HD | P
720 | 1280 | 59.94, 60 | 60 Hz HD | P

The resolution is defined by the equipment configuration, and is reflected in the SDP object.

##### L.4.2.1.2 Connection Policies

###### L.4.2.1.2.1 General

The consumer shall get the SDP object on the following URL: http://<local-IP-address-of-the-device>/SDP.

###### L.4.2.1.2.2 Number of Connections

L.4.2.1.2.2

EXAMPLE-RTV-SERVICE is provided in multicast. The limit of simultaneous connection depends on the local network infrastructure.

Prev | Up | Next
L.4 Networking | Home | L.4.3 Network Interfaces

DICOM PS3.2 2021d - Conformance