DICOM PS3.11 2021d - Media Storage Application Profiles

J.3.4 Other Parameters (Current)
Prev | J.3 STD-GEN-USB, STD-GEN-SEC-USB, STD-GEN-MMC, STD-GEN-SEC-MMC, STD-GEN-CF, STD-GEN-SEC-CF, STD-GEN-SD and STD-GEN-SEC-SD Profile Classes | Next

### J.3.4 Other Parameters

#### J.3.4.2 Multi-frame JPEG Format

The JPEG encoding of pixel data shall use Interchange Format (with table specification) for all frames.

Prev | Up | Next
J.3.3 Directory Information in DICOMDIR | Home | J.3.5 Security Parameters

DICOM PS3.11 2021d - Media Storage Application Profiles