DICOM PS3.16 2021d - Content Mapping Resource

TID 10053 Patient Attenuation Characteristics (Current)
Prev | Enhanced X-Ray Radiation Dose SR IOD Templates | Next

### TID 10053 Patient Attenuation Characteristics

This template describes the details of the patient attenuation characteristics that may be determined/used by the system (e.g., patient equivalent thickness, water equivalent diameter, etc.).

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 10053. Patient Attenuation Characteristics

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (130529, DCM, "Patient Attenuation Characteristics") | 1 | M |  |
2 | > | CONTAINS | DATETIME | DT (111526, DCM, "DateTime Started") | 1 | M |  |
3 | > | CONTAINS | DATETIME | DT (111527, DCM, "DateTime Ended") | 1 | M |  |
4 | > | CONTAINS | TEXT | EV (113832, DCM, "Identification of the X-Ray Source") | 1 | M |  |
5 | > | CONTAINS | NUM | EV (111638, DCM, "Patient Equivalent Thickness") | 1 | UC | XOR Row 6 | UNITS = EV (mm, UCUM, "mm")
6 | > | CONTAINS | TABLE | EV (111638, DCM, "Patient Equivalent Thickness") | 1 | UC | XOR Row 5 | NCOLUMNS = 2 COLUMN 1 = EV (111526, DCM, "DateTime Started") COLUMN 2 = EV (111638, DCM, "Patient Equivalent Thickness") COLUMN 2 UNITS = EV (mm, UCUM, "mm") COLUMN 1 VR = DT COLUMN 2 VR = FL
7 | > | CONTAINS | NUM | EV (113980, DCM, "Water Equivalent Diameter") | 1 | UC | XOR Row 8 | UNITS = EV (mm, UCUM, "mm")
8 | > | CONTAINS | TABLE | EV (113980, DCM, "Water Equivalent Diameter") | 1 | UC | XOR Row 7 | NCOLUMNS = 2 COLUMN 1 = EV (111526, DCM, "DateTime Started") COLUMN 2 = EV (113980, DCM, "Water Equivalent Diameter") COLUMN 2 UNITS = EV (mm, UCUM, "mm") COLUMN 1 VR = DT COLUMN 2 VR = FL
9 | > | CONTAINS | NUM | EV (113931, DCM, "Measured Lateral Dimension") | 1 | UC | XOR Row 10 | UNITS = EV (mm, UCUM, "mm")
10 | > | CONTAINS | TABLE | EV (113931, DCM, "Measured Lateral Dimension") | 1 | UC | XOR Row 9 | NCOLUMNS = 2 COLUMN 1 = EV (111526, DCM, "DateTime Started") COLUMN 2 = EV (113931, DCM, "Measured Lateral Dimension") COLUMN 2 UNITS = EV (mm, UCUM, "mm") COLUMN 1 VR = DT COLUMN 2 VR = FL
11 | > | CONTAINS | NUM | EV (113932, DCM, "Measured AP Dimension") | 1 | UC | XOR Row 12 | UNITS = EV (mm, UCUM, "mm")
12 | > | CONTAINS | TABLE | EV (113932, DCM, "Measured AP Dimension") | 1 | UC | XOR Row 11 | NCOLUMNS = 2 COLUMN 1 = EV (111526, DCM, "DateTime Started") COLUMN 2 = EV (113932, DCM, "Measured AP Dimension") COLUMN 2 UNITS = EV (mm, UCUM, "mm") COLUMN 1 VR = DT COLUMN 2 VR = FL
13 | > | CONTAINS | NUM | EV (113933, DCM, "Derived Effective Diameter") | 1 | UC | XOR Row 14 | UNITS = EV (mm, UCUM, "mm")
14 | > | CONTAINS | TABLE | EV (113933, DCM, "Derived Effective Diameter") | 1 | UC | XOR Row 13 | NCOLUMNS = 2 COLUMN 1 = EV (111526, DCM, "DateTime Started") COLUMN 2 = EV (113933, DCM, "Derived Effective Diameter") COLUMN 2 UNITS = EV (mm, UCUM, "mm") COLUMN 1 VR = DT COLUMN 2 VR = FL
15 | > | CONTAINS | CODE | EV (129715009, SCT, "Breast composition") | 1 | UC | XOR Row 16 | DCID 6000 “Overall Breast Composition”
16 | > | CONTAINS | TABLE | EV (129715009, SCT, "Breast composition") | 1 | UC | XOR Row 15 | NCOLUMNS = 2 COLUMN 1 = EV (111526, DCM, "DateTime Started") COLUMN 2 = EV (129715009, SCT, "Breast composition") COLUMN 2 VALUES = DCID 6000 “Overall Breast Composition” COLUMN 1 VR = DT COLUMN 2 VR = SQ

Content Item Descriptions

Row 2 | The DateTime of the beginning of the time period over which the content items are applicable.
Row 3 | The DateTime of the end of the time period over which the content items are applicable.
Row 4 | Identification the X-Ray source. This designation shall not change for a given source throughout the entire RDSR. For systems with multiple X-Ray sources, each source shall be described with a separate instance of this template.
Row 5-16 | Patient-specific measurements which may be determined by the imaging equipment during the scope of accumulation. If they are known, they may be reported here.

Prev | Up | Next
TID 10052 Attenuator Position | Home | TID 10054 Procedure Characteristics

DICOM PS3.16 2021d - Content Mapping Resource