V.3 Chest X-Ray Hanging Protocol Example
Prev | V Hanging Protocols (Informative) | Next

## V.3 Chest X-Ray Hanging Protocol Example

Goal: A Hanging Protocol for Chest X-ray, PA & Lateral (LL, RL) views, current & prior, with the following layout:

Figure V.3-1. Chest X-Ray Hanging Protocol Example

The Hanging Protocol Definition does not specify a specific modality, but rather a specific anatomy (Chest). The Image Sets Sequence provides more detail, in that it specifies the modalities in addition to the anatomy for each image set.

### V.3.1 Hanging Protocol Definition Module

- Hanging Protocol Name: "Chest X-ray"

- Hanging Protocol Description: "Current and Prior Chest PA and Lateral"

- Hanging Protocol Level: "SITE"

- Hanging Protocol Creator: "Senior Radiologist"

- Hanging Protocol Creation DateTime: "20020823133455"

- Hanging Protocol Definition Sequence:

  - Item 1:

  - Anatomic Region Sequence:

    - Item 1: (T-D3000, SRT, "Chest")

  - Laterality: zero length

  - Procedure Code Sequence: zero length

  - Reason for Requested Procedure Code Sequence: zero length

- Number of Priors Referenced: 1

- Image Sets Sequence:

  - Item 1:

    - Image Set Selector Sequence:

      - Item 1:

        - Image Set Selector Usage Flag: "NO_MATCH"

        - Selector Attribute: (0008,2218) [Anatomic Region Sequence]

        - Selector Attribute VR: "SQ"

        - Selector Code Sequence Value:

          - Item 1: (T-D3000, SRT, "Chest")

        - Selector Value Number: 1

      - Item 2:

        - Image Set Selector Usage Flag: "NO_MATCH"

        - Selector Attribute: (0008,0060) [Modality]

        - Selector Attribute VR: "CS"

        - Selector CS Value: "CR\DX"

        - Selector Value Number: 1

  - Time Based Image Sets Sequence:

    - Item 1:

      - Image Set Number: 1

      - Image Set Selector Category: "RELATIVE_TIME"

      - Relative Time: 0\0

      - Relative Time Units: "MINUTES"

      - Image Set Label: "Current Chest X-ray"

    - Item 2:

      - Image Set Number: 2

      - Image Set Selector Category: "ABSTRACT_PRIOR"

      - Abstract Prior Value: 1\1

      - Image Set Label: "Prior Chest X-ray"

- Hanging Protocol User Identification Code Sequence: zero length

- Hanging Protocol User Group Name: "ABC Hospital"

### V.3.2 Hanging Protocol Environment Module

- Number of Screens: 2

- Nominal Screen Definition Sequence:

  - Item 1:

    - Number of Vertical Pixels: 2560

    - Number of Horizontal Pixels: 2048

    - Display Environment Spatial Position: 0.0\1.0\0.5\0.0, representing (0,1), (0.5,0)

    - Screen Minimum Grayscale Bit Depth: 8

    - Application Maximum Repaint Time: 100

  - Item 2:

    - Number of Vertical Pixels: 2560

    - Number of Horizontal Pixels: 2048

    - Display Environment Spatial Position: 0.5\1.0\1.0\0.0, representing (0.5,1), (1,0)

    - Screen Minimum Grayscale Bit Depth: 8

    - Application Maximum Repaint Time: 100

### V.3.3 Hanging Protocol Display Module

- Display Sets Sequence:

  - Item 1:

    - Display Set Number: 1

    - Display Set Presentation Group: 1

    - Image Set Number: 2

    - Image Boxes Sequence:

      - Item 1:

        - Image Box Number: 1

        - Display Environment Spatial Position: 0.0\1.0\0.25\0.0, representing (0,1), (0.25,0)

        - Image Box Layout Type: "SINGLE"

    - Filter Operations Sequence:

      - o Item 1:

        - Selector Attribute: (0018,5101) [View Position]

        - Selector Attribute VR: "CS"

        - Selector CS Value: "RL\LL"

        - Selector Value Number: 1

        - Filter-by Operator: "MEMBER_OF"

    - Sorting Operations Sequence: zero length

    - Display Set Patient Orientation: "A\F"

    - Show Image True Size Flag: "NO"

    - Show Graphic Annotation Flag: "NO"

  - Item 2:

    - Display Set Number: 2

    - Display Set Presentation Group: 1

    - Image Set Number: 2

    - Image Boxes Sequence:

      - Item 1:

        - Image Box Number: 1

        - Display Environment Spatial Position: 0.25\1.0\0.5\0.0, representing (0.25,1), (0.5,0)

        - Image Box Layout Type: "SINGLE"

    - Filter Operations Sequence:

      - Item 1:

        - Selector Attribute: (0018,5101) [View Position]

        - Selector Attribute VR: "CS"

        - Selector CS Value: "PA"

        - Selector Value Number: 1

        - Filter-by Operator: "MEMBER_OF"

    - Sorting Operations Sequence: zero length

    - Display Set Patient Orientation: "R\F"

    - Show Image True Size Flag: "NO"

    - Show Graphic Annotation Flag: "NO"

  - Item 3:

    - Display Set Number: 3

    - Display Set Presentation Group: 1

    - Image Set Number: 1

    - Image Boxes Sequence:

      - Item 1:

        - Image Box Number: 1

        - Display Environment Spatial Position: 0.5\1.0\0.75\1.0, representing (0.5,1), (0.75,0)

        - Image Box Layout Type: "SINGLE"

    - Filter Operations Sequence:

      - Item 1:

        - Selector Attribute: (0018,5101) [View Position]

        - Selector Attribute VR: "CS"

        - Selector CS Value: "PA"

        - Selector Value Number: 1

        - Filter-by Operator: "MEMBER_OF"

    - Sorting Operations Sequence: zero length

    - Display Set Patient Orientation: "R\F"

    - Show Image True Size Flag: "NO"

    - Show Graphic Annotation Flag: "NO"

  - Item 4:

    - Display Set Number: 4

    - Display Set Presentation Group: 1

    - Image Set Number: 1

    - Image Boxes Sequence:

      - Item 1:

        - Image Box Number: 1

        - Display Environment Spatial Position: 0.75\1.0\1.0\0.0, representing (0.75,1), (1,0)

        - Image Box Layout Type: "SINGLE"

    - Filter Operations Sequence:

      - Item 1:

        - Selector Attribute: (0018,5101) [View Position]

        - Selector Attribute VR: "CS"

        - Selector CS Value: "RL\LL"

        - Selector Value Number: 1

        - Filter-by Operator: "MEMBER_OF"

    - Sorting Operations Sequence: zero length

    - Display Set Patient Orientation: "A\F"

    - Show Image True Size Flag: "NO"

    - Show Graphic Annotation Flag: "NO"

- Partial Data Display Handling: "MAINTAIN_LAYOUT"

Prev | Up | Next
V.2 Hanging Protocol Internal Process Model | Home | V.4 Neurosurgery Planning Hanging Protocol Example