Quantitative Ventricular Analysis Report SR IOD Templates
Prev | A Structured Reporting Templates (Normative) | Next

## Quantitative Ventricular Analysis Report SR IOD Templates

The templates that comprise the Quantitative Ventricular Analysis SR are interconnected as in Figure A-3:

Figure A-3. Quantitative Ventricular Analysis Report SR IOD Template Structure

### TID 3202 Ventricular Analysis

The Ventricular Analysis Template provides a CONTAINER with a structure for reporting the result of the ventricular analysis.

Type:

  Extensible

Order:

  Significant

Table TID 3202. Ventricular Analysis

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (122292, DCM, "Quantitative Ventriculography Report") | 1 | M |  |
2 | > | HAS CONCEPT MOD | INCLUDE | DTID 1204 “Language of Content Item and Descendants” | 1 | M |  |
3 | > | HAS OBS CONTEXT | INCLUDE | DTID 1002 “Observer Context” | 1-n | M |  |
4 | > | CONTAINS | INCLUDE | DTID 3602 “Cardiovascular Patient Characteristics” | 1 | U |  |
5 | > | CONTAINS | CONTAINER | EV (122144, DCM, "Quantitative Analysis") | 1-n | M |  |
6 | >> | HAS OBS CONTEXT | INCLUDE | DTID 1002 “Observer Context” | 1-n | U |  |
7 | >> | HAS OBS CONTEXT | TEXT | EV (111001, DCM, "Algorithm Name") | 1 | M |  |
8 | >> | HAS OBS CONTEXT | TEXT | EV (111003, DCM, "Algorithm Version") | 1 | M |  |
9 | >> | HAS OBS CONTEXT | TEXT | EV (122405, DCM, "Algorithm Manufacturer") | 1 | M |  |
10 | >> | CONTAINS | IMAGE | EV (121112, DCM, "Source of Measurement") | 1-n | M |  |
11 | >>> | HAS CONCEPT MOD | CODE | EV (G-A60B, SRT, "Cardiac Phase") | 1 | M |  | DCID 12233 “Cardiac Phase”
12 | >>> | HAS CONCEPT MOD | CODE | EV (111031, DCM, "Image View") | 1 | MC | If Biplane Analysis | DCID 3466 “Plane Identification”
13 | >> | HAS ACQ CONTEXT | INCLUDE | DTID 3205 “Calibration” | 1-2 | U | VM = 1: Single plane analysis, VM = 2: Biplane analysis | $CalibrationPlane = DCID 3466 “Plane Identification”
14 | >> | HAS ACQ CONTEXT | INCLUDE | DTID 3520 “Hemodynamic Clinical Context” | 1 | U |  |
15 | >> | CONTAINS | INCLUDE | DTID 3206 “VA Main Results” | 1 | M |  |
16 | >> | CONTAINS | INCLUDE | DTID 3207 “AA Main Results” | 1 | U |  |
17 | >> | CONTAINS | INCLUDE | DTID 3208 “Frame-to-Frame Results” | 1 | U |  |
18 | >> | CONTAINS | INCLUDE | DTID 3209 “Centerline Wall Motion” | 1-2 | U | VM = 1: Single plane analysis, VM = 2: Biplane analysis |
19 | >> | CONTAINS | INCLUDE | DTID 3210 “Radial Based Wall Motion” | 1-2 | U | VM = 1: Single plane analysis, VM = 2: Biplane analysis |
20 | >> | CONTAINS | INCLUDE | DTID 3211 “Landmark Based Wall Motion” | 1-2 | U | VM = 1: Single plane analysis, VM = 2: Biplane analysis |

Content Item Descriptions

Row 7 | Identifies the Ventricular Analysis program
Row 8 | Identifies the Ventricular Analysis program version
Row 9 | Identifies the Ventricular Analysis program manufacturer
Row 10 | Identifies the ES and ED images on which the analysis is based, for frame by frame analysis the analyzed image are specified in the frame by frame results (3208) template

### TID 3205 Calibration

The Calibration Template consists of a CONTAINER, with a structure for reporting of the calibration of images used in the analysis.

Table TID 3205. Parameters

Parameter Name | Parameter Usage
--- | ---
$CalibrationPlane | XA Imaging plane

Type:

  Extensible

Order:

  Significant

Table TID 3205. Calibration

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (122505, DCM, "Calibration") | 1 | M |  |
2 | > | HAS CONCEPT MOD | CODE | EV (111031, DCM, "Image View") | 1 | U |  | $CalibrationPlane
3 | > | HAS OBS CONTEXT | TEXT | EV (111001, DCM, "Algorithm Name") | 1 | MC | IF different from Analysis program specified in the invoking template |
4 | > | HAS OBS CONTEXT | TEXT | EV (111003, DCM, "Algorithm Version") | 1 | MC | IF different from Analysis program specified in the invoking template |
5 | > | HAS OBS CONTEXT | TEXT | EV (122405, DCM, "Algorithm Manufacturer") | 1 | MC | IF different from Analysis program specified in the invoking template |
6 | > | CONTAINS | CODE | EV (122422, DCM, "Calibration Method") | 1 | M |  | DCID 3452 “Calibration Methods”
7 | > | CONTAINS | CODE | EV (122421, DCM, "Calibration Object") | 1 | MC | If row 6 value specifies Calibration Object Used | DCID 3451 “Calibration Objects”
8 | > | CONTAINS | NUM | EV (122423, DCM, "Calibration Object Size") | 1 | MC | If row 6 value specifies Calibration Object Used | DCID 3510 “Catheter Size Units”
9 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | M |  | $Measurement = EV (111026, DCM, "Horizontal Pixel Spacing") $Unit = DT (mm/{pixel}, UCUM, "mm/pixel") $ImagePurpose = EV (121112, DCM, "Source of Measurement")
10 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | M |  | $Measurement = EV (111066, DCM, "Vertical Pixel Spacing") $Unit = DT (mm/{pixel}, UCUM, "mm/pixel") $ImagePurpose = EV (121112, DCM, "Source of Measurement")
11 | > | CONTAINS | IMAGE | No purpose of reference | 1 | U |  |

Content Item Descriptions

Row 3 | Identifies the Calibration program
Row 4 | Identifies the Calibration program version
Row 5 | Identifies the Calibration program manufacturer
Row 7 | Besides a Sphere and a Catheter, a Distance can be identified as a Calibration Object. In this case a distance measurement of a known dimension of the object is used to calculate the pixel size.
Row 8 | The catheter size units is also used to specify the size of other calibration objects (e.g., sphere)
Row 9, 10 | Spacing in the patient body. Point to a single frame containing the image used for calibration if applicable, the actual measurements may be indicated by a SCOORD (see TID 320 “Image or Spatial Coordinates”, row 3)
Row 11 | Secondary Capture image with calibration position

### TID 3206 VA Main Results

The VA Main Results Template consists of a CONTAINER with a structure for reporting the main ventricular analysis measurements.

Type:

  Extensible

Order:

  Significant

Table TID 3206. VA Main Results

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (121070, DCM, "Findings") | 1 | M |  |
2 | > | HAS CONCEPT MOD | CODE | EV (G-C0E3, SRT, "Finding Site") | 1 | M |  | DCID 3462 “Chamber Identification”
3 | > | CONTAINS | CODE | EV (122429, DCM, "Volume Method") | 1 | M |  | DCID 3453 “Cardiac Volume Methods”
4 | > | CONTAINS | NUM | EV (122435, DCM, "Regression Volume Exponent") | 1 | U |  | Unit = DT (1, UCUM, "no units")
5 | > | CONTAINS | NUM | EV (122431, DCM, "Regression Slope ED") | 1 | U |  | Unit = DT ({ratio}, UCUM, "ratio")
6 | > | CONTAINS | NUM | EV (122432, DCM, "Regression Offset ED") | 1 | U |  | Unit = DT (ml, UCUM, "ml")
7 | > | CONTAINS | NUM | EV (122433, DCM, "Regression Slope ES") | 1 | U |  | Unit = DT ({ratio}, UCUM, "ratio")
8 | > | CONTAINS | NUM | EV (122434, DCM, "Regression Offset ES") | 1 | U |  | Unit = DT (ml, UCUM, "ml")
9 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | M |  | $Measurement = DCID 3467 “Ejection Fraction” $Unit = DT (%, UCUM, "%")
10 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = DCID 3468 “ED Volume” $Unit = DT (ml, UCUM, "ml")
11 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = DCID 3469 “ES Volume” $Unit = DT (ml, UCUM, "ml")
12 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = EV (F-32120, SRT, "Stroke Volume") $Unit = DT (ml, UCUM, "ml")
13 | > | CONTAINS | NUM | EV (8867-4, LN, "Heart Rate") | 1 | U |  | Unit = DT ({H.B.}/min, UCUM, "BPM")
14 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = DCID 3468 “ED Volume” $ModType = EV (121425, DCM, "Index") $ModValue = DCID 3455 “Index Methods” $Unit = DT (ml/m2, UCUM, "ml/m2")
15 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = DCID 3468 “ED Volume” $ModType = EV (121425, DCM, "Index") $ModValue = EV (29463-7, LN, "Patient Weight") $Unit = DT (ml/kg, UCUM, "ml/kg")
16 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = DCID 3469 “ES Volume” $ModType = EV (121425, DCM, "Index") $ModValue = DCID 3455 “Index Methods” $Unit = DT (ml/m2, UCUM, "ml/m2")
17 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = DCID 3469 “ES Volume” $ModType = EV (121425, DCM, "Index") $ModValue = EV (29463-7, LN, "Patient Weight") $Unit = DT (ml/kg, UCUM, "ml/kg")
18 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = EV (F-32120, SRT, "Stroke Volume") $ModType = EV (121425, DCM, "Index") $ModValue = DCID 3455 “Index Methods” $Unit = DT (ml/m2, UCUM, "ml/m2")
19 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = EV (F-32120, SRT, "Stroke Volume") $ModType = EV (121425, DCM, "Index") $ModValue = EV (29463-7, LN, "Patient Weight") $Unit = DT (ml/kg, UCUM, "ml/kg")
20 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = EV (F-32100, SRT, "Cardiac Output") $Unit = DT (l/min, UCUM, "l/min")
21 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = EV (F-32110, SRT, "Cardiac Index") $ModType = EV (121425, DCM, "Index") $ModValue = DCID 3455 “Index Methods” $Unit = DT (l/min/m2, UCUM, "l/min/m2")
22 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = EV (122445, DCM, "Wall Thickness") $Unit = DT (mm, UCUM, "mm")
23 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = EV (122446, DCM, "Wall Volume") $Unit = DT (ml, UCUM, "ml")
24 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = EV (122447, DCM, "Wall Mass") $Unit = DT (g, UCUM, "gram")
25 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = EV (122447, DCM, "Wall Mass") $ModType = EV (121425, DCM, "Index") $ModValue = DCID 3455 “Index Methods” $Unit = DT (g/m2, UCUM, "gram/m2")
26 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = EV (122447, DCM, "Wall Mass") $ModType = EV (121425, DCM, "Index") $ModValue = EV (29463-7, LN, "Patient Weight") $Unit = DT (g/kg, UCUM, "gram/kg")
27 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = EV (122448, DCM, "Wall Stress") $Unit = DT (dyn/cm2, UCUM, "dynes/cm2")
28 | > | CONTAINS | IMAGE | No purpose of reference | 1-n | U |  |

Content Item Descriptions

Row 28 | Secondary Capture image with ED and/or ES contours

### TID 3207 AA Main Results

The AA Main Results Template consists of a CONTAINER with a structure for reporting the main atrial analysis measurements.

Type:

  Extensible

Order:

  Significant

Table TID 3207. AA Main Results

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (121070, DCM, "Findings") | 1 | M |  |
2 | > | HAS CONCEPT MOD | CODE | EV (G-C0E3, SRT, "Finding Site") | 1 | M |  | DCID 3462 “Chamber Identification”
3 | > | CONTAINS | CODE | EV (122429, DCM, "Volume Method") | 1 | M |  | DCID 3453 “Cardiac Volume Methods”
4 | > | CONTAINS | NUM | EV (122435, DCM, "Regression Volume Exponent") | 1 | U |  | Unit = DT (1, UCUM, "no units")
5 | > | CONTAINS | NUM | EV (122431, DCM, "Regression Slope ED") | 1 | U |  | Unit = DT ({ratio}, UCUM, "ratio")
6 | > | CONTAINS | NUM | EV (122432, DCM, "Regression Offset ED") | 1 | U |  | Unit = DT (ml, UCUM, "ml")
7 | > | CONTAINS | NUM | EV (122433, DCM, "Regression Slope ES") | 1 | U |  | Unit = DT ({ratio}, UCUM, "ratio")
8 | > | CONTAINS | NUM | EV (122434, DCM, "Regression Offset ES") | 1 | U |  | Unit = DT (ml, UCUM, "ml")
9 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = DCID 3468 “ED Volume” $Unit = DT (ml, UCUM, "ml")
10 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = DCID 3469 “ES Volume” $Unit = DT (ml, UCUM, "ml")
11 | > | CONTAINS | IMAGE | No purpose of reference | 1-n | U |  |

Content Item Descriptions

Row 11 | Secondary Capture image with ED and/or ES contours

### TID 3208 Frame-to-Frame Results

The Frame-to-Frame Result Template consists of a CONTAINER providing measurements derived from the angiographic images on frame-by-frame basis.

Type:

  Extensible

Order:

  Significant

Table TID 3208. Frame-To-Frame Result

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (121070, DCM, "Findings") | 1 | M |  |
2 | > | HAS CONCEPT MOD | CODE | EV (111004, DCM, "Analysis Performed") | 1 | M |  | EV (122499, DCM, "Frame to Frame Analysis")
3 | > | CONTAINS | IMAGE | EV (121112, DCM, "Source of Measurement") | 1-2 | M | VM = 1: Single plane analysis, VM = 2: Biplane analysis |
4 | > | CONTAINS | CODE | EV (122429, DCM, "Volume Method") | 1 | M |  | DCID 3453 “Cardiac Volume Methods”
5 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1-n | M |  | $Measurement = DCID 3471 “Estimated Volumes” $TargetSite = DCID 3462 “Chamber Identification” $Unit = DT (ml, UCUM, "ml")
6 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1-n | U |  | $Measurement = EV (122445, DCM, "Wall Thickness") $Unit = DT (mm, UCUM, "mm")
7 | > | CONTAINS | IMAGE | No purpose of reference | 1-n | U |  |

Content Item Descriptions

Row 3 | Identifies each frame analyzed, using the multi-valued Referenced Frame Number (0008,1160) attribute of the IMAGE content item.
Row 5, 6 | Includes one measurement for each frame referenced in Row 3.
Row 7 | Secondary Capture image with ventricular contours

### TID 3209 Centerline Wall Motion

The Centerline Wall Motion Template consists of a CONTAINER providing measurements of the centerline wall motion.

Type:

  Extensible

Order:

  Significant

Table TID 3209. Centerline Wall Motion

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (121070, DCM, "Findings") | 1 | M |  |
2 | > | HAS CONCEPT MOD | CODE | EV (111004, DCM, "Analysis Performed") | 1 | M |  | EV (122449, DCM, "Centerline Wall Motion Analysis")
3 | >> | HAS CONCEPT MOD | CODE | EV (122410, DCM, "Contour Realignment") | 1 | M |  | DCID 3458 “Contour Realignment”
4 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 100 | M |  | $Measurement = EV (122450, DCM, "Normalized Chord Length") $Unit = DT (%, UCUM, "%")
5 | > | CONTAINS | NUM | EV (122411, DCM, "Threshold Value") | 1 | M |  | Values shall be 1, 2 or 3 UNITS = EV ({sd}, UCUM, "Standard Deviations")
6 | > | CONTAINS | CONTAINER | EV (122451, DCM, "Abnormal Region") | 1-6 | U |  |
7 | >> | CONTAINS | CODE | EV (F-32050, SRT, "Cardiac Wall Motion") | 1 | M |  | DCID 3703 “Wall Motion”
8 | >> | CONTAINS | CODE | EV (R-404F0, SRT, "Circumferential Extent") | 1 | U |  | DCID 3460 “Circumferential Extent”
9 | >> | CONTAINS | NUM | EV (122452, DCM, "First Chord of Abnormal Region") | 1 | M |  | Unit = DT (1, UCUM, "no unit")
10 | >> | CONTAINS | NUM | EV (122453, DCM, "Last Chord of Abnormal Region") | 1 | M |  | Unit = DT (1, UCUM, "no unit")
11 | > | CONTAINS | CONTAINER | EV (122417, DCM, "Regional Abnormal Wall Motion ") | 1-4 | U |  |
12 | >> | HAS CONCEPT MOD | CODE | EV (G-C03E, SRT, "Finding Site") | 1 | M |  | DCID 3461 “Regional Extent”
13 | >> | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | M |  | $Measurement = EV (122459, DCM, "Territory Region Severity") $ModType = EV (F-32050, SRT, "Cardiac Wall Motion") $ModValue = DCID 3703 “Wall Motion” $Unit = DT ({sd}, UCUM, "Standard Deviations")
14 | >> | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | M |  | $Measurement = EV (122461, DCM, "Opposite Region Severity") $ModType = EV (F-32050, SRT, "Cardiac Wall Motion") $ModValue = DCID 3703 “Wall Motion” $Unit = DT ({sd}, UCUM, "Standard Deviations")
15 | > | CONTAINS | IMAGE | No purpose of reference | 1 | U |  |

Content Item Descriptions

Row 4 | Normalized lengths of the chords determined between ED and ES contour. The measurement template allows the specification of the statistical properties of the normal population and of the chord measurement relative to the population.
Row 8 | If the Circumferential Extent is not specified no limitations to the boundaries for regions are assumed.
Row 11 | The Regional Abnormal Wall Motion container holds the information on the severity of the decreased or increased wall motion of the 4 predefined regions as described in [Sheehan, 1986].
Row 12 | The name of the region with an abnormal ventricular wall motion as described in [Sheehan, 1986].
Row 13 | The severity of the wall motion abnormality expressed in Standard Deviations above or below normal in the territory region as described in [Sheehan, 1986].
Row 14 | The severity of the wall motion abnormality expressed in Standard Deviations above or below normal in the opposite region as described in [Sheehan, 1986].
Row 15 | Secondary Capture image with centerline analysis result

### TID 3210 Radial Based Wall Motion

The Radial Based Wall Motion Template consists of a CONTAINER providing measurements of the radial based wall motion.

Type:

  Extensible

Order:

  Significant

Table TID 3210. Radial Based Wall Motion

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (121070, DCM, "Findings") | 1 | M |  |
2 | > | HAS CONCEPT MOD | CODE | EV (111004, DCM, "Analysis Performed") | 1 | M |  | EV (122493, DCM, "Radial Based Wall Motion Analysis")
3 | >> | HAS CONCEPT MOD | CODE | EV (122410, DCM, "Contour Realignment") | 1 | M |  | DCID 3458 “Contour Realignment”
4 | > | CONTAINS | CONTAINER | EV (121070, DCM, "Findings") | 1-n | M |  |
5 | >> | HAS CONCEPT MOD | CODE | EV (G-C0E3, SRT, "Finding Site") | 1 | M |  | DCID 3718 “Myocardial Wall Segments in Projection”
6 | >> | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | M |  | $Measurement = EV (122495, DCM, "Regional Contribution to Ejection Fraction") $Unit = DT (%, UCUM, "%")
7 | >> | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1-n | U |  | $Measurement = EV (122496, DCM, "Radial Shortening") $Unit = DT (%, UCUM, "%")
8 | > | CONTAINS | IMAGE | No purpose of reference | 1 | U |  |

Content Item Descriptions

Row 6 | The CREF values of the 6 regions determined for the radial based wall motion
Row 7 | The shortening of the measured radials within the region
Row 8 | Secondary Capture image with radial based analysis result

### TID 3211 Landmark Based Wall Motion

The Landmark Based Wall Motion Template consists of a CONTAINER providing measurements of the landmark based wall motion.

Type:

  Extensible

Order:

  Significant

Table TID 3211. Landmark Based Wall Motion

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (121070, DCM, "Findings") | 1 | M |  |
2 | > | HAS CONCEPT MOD | CODE | EV (111004, DCM, "Analysis Performed") | 1 | M |  | EV (122497, DCM, "Landmark Based Wall Motion Analysis")
3 | >> | HAS CONCEPT MOD | CODE | EV (122410, DCM, "Contour Realignment") | 1 | M |  | DCID 3458 “Contour Realignment”
4 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1-n | M |  | $Measurement = EV (122498, DCM, "Slice Contribution to Ejection Fraction") $Unit = DT (%, UCUM, "%")
5 | > | CONTAINS | CONTAINER | EV (121070, DCM, "Findings") | 5 | M |  |
6 | >> | HAS CONCEPT MOD | CODE | EV (G-C0E3, SRT, "Finding Sites") | 1 | M |  | DCID 3718 “Myocardial Wall Segments in Projection”
7 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | M |  | $Measurement = EV (122495, DCM, "Regional Contribution to Ejection Fraction") $Unit = DT (%, UCUM, "%")
8 | > | CONTAINS | IMAGE | No purpose of reference | 1 | U |  |

Content Item Descriptions

Row 8 | Secondary Capture image with Landmark Based Analysis result

Prev | Up | Next
Procedure Log IOD Templates | Home | Quantitative Arterial Analysis Report SR IOD Templates