TID 3211 Landmark Based Wall Motion
Prev | Quantitative Ventricular Analysis Report SR IOD Templates | Next

### TID 3211 Landmark Based Wall Motion

The Landmark Based Wall Motion Template consists of a CONTAINER providing measurements of the landmark based wall motion.

Type:

  Extensible

Order:

  Significant

Table TID 3211. Landmark Based Wall Motion

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (121070, DCM, "Findings") | 1 | M |  |
2 | > | HAS CONCEPT MOD | CODE | EV (111004, DCM, "Analysis Performed") | 1 | M |  | EV (122497, DCM, "Landmark Based Wall Motion Analysis")
3 | >> | HAS CONCEPT MOD | CODE | EV (122410, DCM, "Contour Realignment") | 1 | M |  | DCID 3458 “Contour Realignment”
4 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1-n | M |  | $Measurement = EV (122498, DCM, "Slice Contribution to Ejection Fraction") $Unit = DT (%, UCUM, "%")
5 | > | CONTAINS | CONTAINER | EV (121070, DCM, "Findings") | 5 | M |  |
6 | >> | HAS CONCEPT MOD | CODE | EV (G-C0E3, SRT, "Finding Sites") | 1 | M |  | DCID 3718 “Myocardial Wall Segments in Projection”
7 | > | CONTAINS | INCLUDE | DTID 300 “Measurement” | 1 | M |  | $Measurement = EV (122495, DCM, "Regional Contribution to Ejection Fraction") $Unit = DT (%, UCUM, "%")
8 | > | CONTAINS | IMAGE | No purpose of reference | 1 | U |  |

Content Item Descriptions

Row 8 | Secondary Capture image with Landmark Based Analysis result

Prev | Up | Next
TID 3210 Radial Based Wall Motion | Home | Quantitative Arterial Analysis Report SR IOD Templates