TID 4021 Mammography CAD Geometry
Prev | Mammography CAD SR IOD Templates | Next

### TID 4021 Mammography CAD Geometry

All geometry template invocations require specification of the location of the center of the object. Outline is optional.

Type:

  Non-Extensible

Order:

  Significant

Table TID 4021. Mammography CAD Geometry

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | SCOORD | EV (111010, DCM, "Center") | 1 | M |  | GRAPHIC TYPE = {POINT}
2 | > | R-SELECTED FROM | IMAGE |  | 1 | M |  | Shall reference an IMAGE content item in the (111028, DCM, "Image Library")
3 |  |  | SCOORD | EV (111041, DCM, "Outline") | 1 | U |  |
4 | > | R-SELECTED FROM | IMAGE |  | 1 | M |  | Shall reference the same content item as row 2
5 |  |  | SCOORD | DCID 6166 “CAD Geometry Secondary Graphical Representation” | 1-n | U |  |
6 | > | R-SELECTED FROM | IMAGE |  | 1 | M |  | Shall reference the same content item as row 2

Prev | Up | Next
TID 4020 CAD Image Library Entry | Home | TID 4022 CAD Observation Context