TID 10006 Accumulated Cassette-based Projection Radiography Dose
Prev | X-Ray Radiation Dose SR IOD Templates | Next

### TID 10006 Accumulated Cassette-based Projection Radiography Dose

This template provides information on Projection Radiography dose values accumulated on Cassette-based systems over one or more irradiation events (typically a study or a performed procedure step) from the same equipment.

Type:

  Extensible

Order:

  Non-Significant

Table TID 10006. Accumulated Cassette-Based Projection Radiography Dose

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CODE | EV (113947, DCM, "Detector Type") | 1 | MC | IF TID (10001) Row 8 is absent or value is (R-0038D, SRT, "Yes") | DCID 10030 “Detector Types”
2 |  |  | NUM | EV (113731, DCM, "Total Number of Radiographic Frames") | 1 | MC | IF TID (10001) Row 8 is absent or value is (R-0038D, SRT, "Yes") | UNITS = EV (1, UCUM, "no units")

Content Item Descriptions

Row 2 | The number of radiographic frames recorded by the X-Ray detector or the number of exposures recorded by the X-Ray source, whichever is known to be greater.

Prev | Up | Next
TID 10005 Accumulated Mammography X-Ray Dose | Home | TID 10007 Accumulated Total Projection Radiography Dose