TID 5202 Echo Section
Prev | Echocardiography Procedure Report Templates | Next

### TID 5202 Echo Section

This is a generic section heading Template for any of the anatomical headings. Measurements within a section heading appear as groups (by image mode, acquisition protocol, and/or protocol stage).

Table TID 5202. Parameters

Parameter Name | Parameter Usage
--- | ---
$SectionSubject | The subject modifier of the section heading container
$MeasType | The concept name of the measurement

Type:

  Extensible

Order:

  Significant

Table TID 5202. Echo Section

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (121070, DCM, "Findings") | 1 | M |  |
2 | > | HAS CONCEPT MOD | CODE | EV (G-C0E3, SRT, "Finding Site") | 1 | M |  | $SectionSubject
3 | > | CONTAINS | CONTAINER | DT (125007, DCM, "Measurement Group") | 1-n | M |  |
4 | >> | HAS CONCEPT MOD | CODE | EV (G-0373, SRT, "Image Mode") | 1 | U |  | BCID 12224 “Ultrasound Image Modes”
5 | >> | HAS CONCEPT MOD | CODE | DT (125203, DCM, "Acquisition Protocol") | 1 | U |  |
6 | >> | HAS CONCEPT MOD | TEXT | DT (125203, DCM, "Acquisition Protocol") | 1 | U |  |
7 | >> | HAS ACQ CONTEXT | CODE | EV (18139-6, LN, "Stage") | 1 | U |  | BCID 12002 “Ultrasound Protocol Stage Types”
8 | >> | CONTAINS | INCLUDE | DTID 5203 “Echo Measurement” | 1-n | M |  | $Measurement = $MeasType $Method = CID 12227 “Echocardiography Measurement Method”

Content Item Descriptions

Rows 4, 5 | Type of measurement group. May be grouped by image mode, or acquisition protocol, or some other user or manufacturer designated classification
Row 7 | For measurements acquired in a staged protocol, all measurements in a measurement group are acquired at the identified stage.

Prev | Up | Next
TID 5201 Echocardiography Patient Characteristics | Home | TID 5203 Echo Measurement