A.33.3 Pseudo-color Softcopy Presentation State IOD
Prev | A.33 Softcopy Presentation State Information Object Definitions | Next

### A.33.3 Pseudo-color Softcopy Presentation State IOD

#### A.33.3.1 Pseudo-color Softcopy Presentation State IOD Description

The Pseudo-Color Softcopy Presentation State Information Object Definition (IOD) specifies information that may be used to present (display) images that are referenced from within the IOD.

It includes capabilities for specifying:

1. the output color space in PCS-Values

2. grayscale contrast transformations including modality and VOI LUT

3. a color palette to map the transformed grayscale values into pseudo-color

4. mask subtraction for multi-frame images

5. selection of the area of the image to display and whether to rotate or flip it

6. image and display relative annotations, including graphics, text and overlays

Prev | Up | Next
A.33.2.2 Color Softcopy Presentation State IOD Module Table | Home | A.33.3.2 Pseudo-color Softcopy Presentation State IOD Module Table