A.44 Hanging Protocol IOD
Prev | A Composite Information Object Definitions (Normative) | Next

## A.44 Hanging Protocol IOD

### A.44.1 Hanging Protocol IOD Description

A Hanging Protocol entity specifies the viewing preferences of a specific user or group, for a specific type of study (Modality, Anatomy, Laterality combination, and optionally Procedure, and/or Reason), that may be exchanged between connecting devices that claim conformance to the DICOM Standard. The Hanging Protocol contains information about the Hanging Protocol, the creator, the type of study it addresses, the type of image sets to display, the intended display environment, and the intended layout for the screen(s).

Prev | Up | Next
A.43.2 Stereometric Relationship IOD Modules | Home | A.44.2 Hanging Protocol IOD Entity-Relationship Model