A.49.2 IOD Modules
Prev | A.49 RT Ion Plan IOD | Next

### A.49.2 IOD Modules

Table A.49-1 identifies and defines the Modules that comprise this IOD. Modules listed are either mandatory or optional as specified in PS3.4. Mandatory Modules contain Attributes that are included in all SOP Instances employing this IOD.

Table A.49-1. RT Ion Plan IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | RT Series | C.8.8.1 | M
Clinical Trial Series | C.7.3.2 | U
Frame of Reference | Frame of Reference | C.7.4.1 | M
Equipment | General Equipment | C.7.5.1 | M
Plan | RT General Plan | C.8.8.9 | M
RT Prescription | C.8.8.10 | U
RT Ion Tolerance Tables | C.8.8.24 | U
RT Patient Setup | C.8.8.12 | U
RT Fraction Scheme | C.8.8.13 | U
RT Ion Beams | C.8.8.25 | C - Required if RT Fraction Scheme Module is included and Number of Beams (300A,0080) is greater than zero for one or more fraction groups
Approval | C.8.8.16 | U
SOP Common | C.12.1 | M
Common Instance Reference | C.12.2 | U

Prev | Up | Next
A.49 RT Ion Plan IOD | Home | A.50 RT Ion Beams Treatment Record IOD