DICOM PS3.11 2016a - Media Storage Application Profiles

H.3.2 Physical Medium and Medium Format
Prev | H.3 STD-GEN-DVD and STD-GEN-SEC-DVD Profile Classes | Next

### H.3.2 Physical Medium and Medium Format

The STD-GEN-DVD and STD-GEN-SEC-DVD application profiles require any of the 120 mm DVD media other than DVD-RAM, as defined in PS3.12.

Prev | Up | Next
H.3 STD-GEN-DVD and STD-GEN-SEC-DVD Profile Classes | Home | H.3.3 Directory Information in DICOMDIR

DICOM PS3.11 2016a - Media Storage Application Profiles