DICOM PS3.2 2016a - Conformance

I.4.2.2.4 Connection Policies
Prev | I.4.2.2 WADO-URI Specification | Next

##### I.4.2.2.4 Connection Policies

###### I.4.2.2.4.1 General

All URI connections are limited to HTTP GET requests. The EXAMPLE-WADO-SERVICE ignores all unknown HTTP header parameters.

###### I.4.2.2.4.2 Number of Connections

EXAMPLE-WADO-SERVICE limits the number of simultaneous HTTP connections.

Table I.4.2-7. Number of HTTP Requests Supported

Maximum number of simultaneous HTTP requests | 100 (configurable)

###### I.4.2.2.4.3 Asynchronous Nature

EXAMPLE-WADO-SERVICE supports HTTP pipelined requests and responses.

Prev | Up | Next
I.4.2.2.3 WADO-URI Retrieve Imaging Document Set Metadata | Home | I.4.2.3 WADO-RS Specifications

DICOM PS3.2 2016a - Conformance