DICOM PS3.18 2016a - Web Services

6.2 WADO-URI Request
Prev | 6 Data Communication Requirements | Next

## 6.2 WADO-URI Request

The HTTP Request used shall use the GET method as defined in [RFC 7230].

### 6.2.1 Parameters of the HTTP Request

The parameters of the <query> component of the Request-URI to be sent to the web Server through the HTTP GET method request shall be represented as defined in [RFC 3986].

### Note

1. Other components of the Request-URI depend on the configuration, e.g., location and script language of the Web Enabled DICOM Server.

2. The means by which the Web Client System obtains the value of the necessary parameters for web accessing of DICOM objects is out of the scope of the standard.

Prev | Up | Next
6 Data Communication Requirements | Home | 6.2.2 Media Types Acceptable in the Response

DICOM PS3.18 2016a - Web Services