DICOM PS3.11 2016a - Media Storage Application Profiles

E.3.2 Physical Medium and Medium Format
Prev | E.3 STD-CTMR Profiles | Next

### E.3.2 Physical Medium and Medium Format

The STD-CTMR-MOD41 application profile requires the 130 mm 4.1GB R/W MOD physical medium with the PCDOS Media Format, as defined in PS3.12.

The STD-CTMR-CD application profile requires the 120 mm CD-R physical medium with the ISO 9660 Media Format, as defined in PS3.12.

The STD-CTMR-DVD-RAM application profile requires the 120 mm DVD-RAM medium, as defined in PS3.12.

The STD-CTMR-DVD application profile requires any of the 120 mm DVD media other than DVD-RAM, as defined in PS3.12.

Prev | Up | Next
E.3 STD-CTMR Profiles | Home | E.3.3 Directory Information in DICOMDIR

DICOM PS3.11 2016a - Media Storage Application Profiles