DICOM PS3.11 2016a - Media Storage Application Profiles

A.3.2 Physical Media and Media Formats
Prev | A.3 STD-XABC-CD Basic Cardiac Profile | Next

### A.3.2 Physical Media and Media Formats

Basic Cardiac Application Profiles in the STD-XABC class require the 120 mm CD-R physical media with the ISO/IEC 9660 Media Format, as defined in PS3.12.

Prev | Up | Next
A.3 STD-XABC-CD Basic Cardiac Profile | Home | A.3.3 Directory Information in DICOMDIR

DICOM PS3.11 2016a - Media Storage Application Profiles