DICOM PS3.3 2016b - Information Object Definitions

C.8.13.5.8 MR Transmit Coil Macro
Prev | C.8.13.5 Enhanced MR Image Functional Group Macros | Next

##### C.8.13.5.8 MR Transmit Coil Macro

Table C.8-95 specifies the attributes of the MR Transmit Coil Functional Group Macro.

Table C.8-95. MR Transmit Coil Macro Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
MR Transmit Coil Sequence | (0018,9049) | 1 | A sequence that provides information about the transmit coil used. Only a single Item shall be included in this Sequence.
>Transmit Coil Name | (0018,1251) | 1C | Name of transmit coil used. Required if Frame Type (0008,9007) Value 1 of this frame is ORIGINAL. May be present otherwise.
>Transmit Coil Manufacturer Name | (0018,9050) | 2C | Name of manufacturer of transmit coil. Required if Frame Type (0008,9007) Value 1 of this frame is ORIGINAL. May be present otherwise.
>Transmit Coil Type | (0018,9051) | 1C | Type of transmit coil used. Required if Frame Type (0008,9007) Value 1 of this frame is ORIGINAL. May be present otherwise. Defined Terms: BODY VOLUME head, extremity, etc. SURFACE

Prev | Up | Next
C.8.13.5.7 MR Receive Coil Macro | Home | C.8.13.5.9 MR Diffusion Macro

DICOM PS3.3 2016b - Information Object Definitions