DICOM PS3.2 2016b - Conformance

B.4.2.3.2 Association Policies
Prev | B.4.2.3 Hardcopy Application Entity Specification | Next

##### B.4.2.3.2 Association Policies

###### B.4.2.3.2.1 General

The DICOM standard application context name for DICOM 3.0 is always proposed:

Table B.4.2-30. DICOM Application Context for AE Hardcopy

Application Context Name | 1.2.840.10008.3.1.1.1

###### B.4.2.3.2.2 Number of Associations

EXAMPLE-INTEGRATED-MODALITY initiates one Association at a time for each configured hardcopy device. Multiple hardcopy devices can be configured.

Table B.4.2-31. Number of Associations Initiated for AE Hardcopy

Maximum number of simultaneous Associations | (number of configured hardcopy devices)

###### B.4.2.3.2.3 Asynchronous Nature

EXAMPLE-INTEGRATED-MODALITY does not support asynchronous communication (multiple outstanding transactions over a single Association).

Table B.4.2-32. Asynchronous Nature as a SCU for AE Hardcopy

Maximum number of outstanding asynchronous transactions | 1

###### B.4.2.3.2.4 Implementation Identifying Information

The implementation information for this Application Entity is:

Table B.4.2-33. DICOM Implementation Class and Version for AE Hardcopy

Implementation Class UID | 1.xxxxxxx.yyy.etc.ad.inf.usw
Implementation Version Name | EXINTMOD_01

Prev | Up | Next
B.4.2.3 Hardcopy Application Entity Specification | Home | B.4.2.3.3 Association Initiation Policy

DICOM PS3.2 2016b - Conformance