DICOM PS3.4 2016b - Service Class Specifications

W.4.4.2 SCP Conformance Requirements
Prev | W.4.4 Conformance Statement Requirements | Next

#### W.4.4.2 SCP Conformance Requirements

An implementation that conforms to the Color Palette Storage SOP Class as an SCP that interprets Color Palette SOP Instances for display shall state in its Conformance Statement:

- The optional Attributes of the Color Palette IOD that it is capable of interpreting and those that are not supported.

- The Image Storage SOP Classes for which application of the Color Palette Storage SOP Class is supported

An implementation that conforms to the Color Palette Storage SOP Class as an SCP shall state in its Conformance Statement:

- The behavior of the SCP in the case of a successful C-STORE operation, including the access method for a stored Color Palette SOP Instance, and the duration of the storage.

- The meaning of each case of a failure C-STORE response status, as well as appropriate recovery action.

Prev | Up | Next
W.4.4 Conformance Statement Requirements | Home | X Color Palette Query/Retrieve Service Class

DICOM PS3.4 2016b - Service Class Specifications