DICOM PS3.16 2016b - Content Mapping Resource

Procedure Log IOD Templates
Prev | A Structured Reporting Templates (Normative) | Next

## Procedure Log IOD Templates

### TID 3001 Procedure Log

The Procedure Log Template is intended for the representation of reports or logs of time-stamped events occurring during an image-guided interventional or other procedure.

This Template does not require a particular ordering of the subsidiary Content Items.

### Note

1. The Procedure Log IOD (PS3.3) requires ordering by Observation DateTime; thus log entries of different types (i.e., specified by different Rows in the Template) may appear in any order.

2. While this Template is extensible, the Procedure Log IOD forbids Container Content Items subsidiary to the top level Container.

Type:

  Extensible

Order:

  Non-Significant

Root:

  Yes

Table TID 3001. Procedure Log

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | DCID 3400 “Procedure Log Titles” | 1 | M |  | Root node
2 | > |  | INCLUDE | DTID 1002 “Observer Context” | 1-n | M |  |
3 | > |  | INCLUDE | DTID 3601 “Procedure Context” | 1 | M |  |
4 | > | HAS ACQ CONTEXT | TEXT | EV (121121, DCM, "Room identification") | 1 | U |  |
5 | > | HAS ACQ CONTEXT | TEXT | EV (121122, DCM, "Equipment identification") | 1-n | U |  |
6 | > | CONTAINS | TEXT | DCID 3401 “Types of Log Notes” | 1-n | U |  |
7 | >> |  | INCLUDE | DTID 3010 “Log Entry Qualifiers” | 1 | U |  |
8 | > | CONTAINS | CODE | EV (121123, DCM, "Patient Status or Event") | 1-n | U |  | DCID 3402 “Patient Status and Events”
9 | >> |  | INCLUDE | DTID 3010 “Log Entry Qualifiers” | 1 | U |  |
10 | > | CONTAINS | PNAME | DCID 3404 “Staff Actions” | 1-n | U |  |
11 | >> |  | INCLUDE | DTID 3010 “Log Entry Qualifiers” | 1 | U |  |
12 | > | CONTAINS | TEXT | DCID 3427 “Equipment Events” | 1-n | U |  | Equipment identifier
13 | >> |  | INCLUDE | DTID 3010 “Log Entry Qualifiers” | 1 | U |  |
14 | > | CONTAINS | INCLUDE | DTID 3100 “Procedure Action” | 1-n | U |  |
15 | > | CONTAINS | INCLUDE | DTID 3101 “Image Acquisition” | 1-n | U |  |
16 | > | CONTAINS | INCLUDE | DTID 3102 “Waveform Acquisition” | 1-n | U |  |
17 | > | CONTAINS | INCLUDE | DTID 3103 “Referenced Object” | 1-n | U |  |
18 | > | CONTAINS | INCLUDE | DTID 3104 “Consumables” | 1-n | U |  |
19 | > | CONTAINS | INCLUDE | DTID 3105 “Lesion Identification and Properties” | 1-n | U |  |
20 | > | CONTAINS | INCLUDE | DTID 3106 “Drugs/Contrast Administered” | 1-n | U |  |
21 | > | CONTAINS | INCLUDE | DTID 3107 “Device Used” | 1-n | U |  |
22 | > | CONTAINS | INCLUDE | DTID 3108 “Intervention” | 1-n | U |  |
23 | > | CONTAINS | CODE | EV (DD-60002, SRT, "Complication of Procedure") | 1-n | U |  | DCID 3413 “Adverse Outcomes”
24 | >> |  | INCLUDE | DTID 3010 “Log Entry Qualifiers” | 1 | U |  |
25 | > | CONTAINS | INCLUDE | DTID 3109 “Measurements” | 1-n | U |  |
26 | > | CONTAINS | INCLUDE | DTID 3110 “Impressions or Findings” | 1-n | U |  |
27 | > | CONTAINS | INCLUDE | DTID 3111 “Percutaneous Entry” | 1-n | U |  |
28 | > | CONTAINS | INCLUDE | DTID 3112 “Specimen Obtained” | 1-n | U |  |
29 | > | CONTAINS | INCLUDE | DTID 3113 “Patient Support” | 1-n | U |  |
30 | > | CONTAINS | INCLUDE | DTID 3114 “Patient Assessment” | 1-n | U |  |
31 | > | CONTAINS | INCLUDE | DTID 3115 “ECG ST Assessment” | 1-n | U |  |

Content Item Descriptions

Row 2 | Includes TID 1002 “Observer Context”, which shall be used to record the identity of the person responsible for recording the log, as well as all other participants in the procedure, even though these personnel may not technically be "observers" of the Procedure Log. As participants in the procedure, they are potential sources for events and observations recorded in the Log. TID 1002 “Observer Context” allows the specification of the person's role in the organization (e.g., physician, nurse), as well as the role in the procedure (e.g., circulating, performing, etc.).
Row 5 | Shall be used to record the identity of the major equipment used in the procedure.
Row 6 | May be used to record any event not covered by a specific log entry Template.

Prev | Up | Next
A Structured Reporting Templates (Normative) | Home | TID 3010 Log Entry Qualifiers

DICOM PS3.16 2016b - Content Mapping Resource