DICOM PS3.16 2016c - Content Mapping Resource

CID 7181 Abstract Multi-dimensional Image Model Component Units
Prev | B DCMR Context Groups (Normative) | Next

## CID 7181 Abstract Multi-dimensional Image Model Component Units

Type:

  Extensible

Version:

  20141110

Table CID 7181. Abstract Multi-dimensional Image Model Component Units

Coding Scheme Designator | Code Value | Code Meaning
--- | --- | ---
Include CID 3500 “Pressure Units”
Include CID 3502 “Hemodynamic Resistance Units”
Include CID 3503 “Indexed Hemodynamic Resistance Units”
Include CID 7460 “Units of Linear Measurement”
Include CID 7461 “Units of Area Measurement”
Include CID 7462 “Units of Volume Measurement”
Include CID 84 “PET Units”
UCUM | 1 | no units
UCUM | {ratio} | ratio
UCUM | [hnsf'U] | Hounsfield Unit
UCUM | {counts} | Counts
UCUM | {counts}/s | Counts per second
UCUM | [arb'U] | arbitrary unit
UCUM | cm/s | centimeter/second
UCUM | mm/s | millimeter/second
UCUM | dB | decibel
UCUM | Cel | degrees Celsius
UCUM | ml/min | milliliter per minute
UCUM | ml/s | milliliter per second
UCUM | ms | millisecond
UCUM | s | second
UCUM | Hz | Hertz
UCUM | mT | milliTesla
UCUM | {Particles}/[100]g{Tissue} | number particles per 100 gram of tissue
UCUM | mm2/s | square millimeter per second
UCUM | s/mm2 | second per square millimeter
UCUM | ml/[100]g/min | milliliter per 100 gram per minute
UCUM | ml/[100]ml | milliliter per 100 milliliter
UCUM | mmol/kg{WetWeight} | millimoles per kg wet weight
UCUM | /min | /min
UCUM | /s | /s

Prev | Up | Next
CID 7180 Abstract Multi-dimensional Image Model Component Semantics | Home | CID 7182 Abstract Multi-dimensional Image Model Dimension Semantics

DICOM PS3.16 2016c - Content Mapping Resource