DICOM PS3.16 2016c - Content Mapping Resource

TID 10007 Accumulated Total Projection Radiography Dose
Prev | X-Ray Radiation Dose SR IOD Templates | Next

### TID 10007 Accumulated Total Projection Radiography Dose

This Template provides information on total Projection Radiography dose values accumulated on Integrated or combined fluoroscopy/acquisition systems over one or more irradiation events (typically a study or a performed procedure step) from the same equipment.

Type:

  Extensible

Order:

  Non-Significant

Root:

  No

Table TID 10007. Accumulated Total Projection Radiography Dose

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | NUM | EV (113722, DCM, "Dose Area Product Total") | 1 | M |  | UNITS = EV (Gy.m2, UCUM, "Gy.m2")
2 |  |  | NUM | EV (113725, DCM, "Dose (RP) Total") | 1 | MC | IF TID (10001) Row 4 = (113958, DCM, "Integrated Projection Radiography System") or any of the values of TID (10001) Row 18 are not (113858, DCM, "MPPS Content"). | UNITS = EV (Gy, UCUM, "Gy")
3 |  |  | NUM | EV (113737, DCM, "Distance Source to Reference Point") | 1 | U |  | UNITS = EV (mm, UCUM, "mm")
4 |  |  | NUM | EV (113731, DCM, "Total Number of Radiographic Frames") | 1 | U |  | UNITS = EV (1, UCUM, "no units")
5 |  |  | CODE | EV (113780, DCM, "Reference Point Definition") | 1 | MC | IF any of (113725, DCM, "Dose (RP) Total"), (113728, DCM, "Fluoro Dose (RP) Total") or (113729, DCM, "Acquisition Dose (RP) Total") are present, and Row 6 is not present. | DCID 10025 “Radiation Dose Reference Points”
6 |  |  | TEXT | EV (113780, DCM, "Reference Point Definition") | 1 | MC | IF any of (113725, DCM, "Dose (RP) Total"), (113728, DCM, "Fluoro Dose (RP) Total") or (113729, DCM, "Acquisition Dose (RP) Total") are present, and Row 5 is not present. |

Content Item Descriptions

Row 1 | Accumulated Dose Area Product
Row 2 | Accumulated dose relative to reference point.
Row 3 | A single value for Radiography systems calculating reference point dose based on fixed distance.
Row 5 | A coded definition of the Reference Point (RP) used for RP-related dose values.
Row 6 | A text definition of the Reference Point (RP) used for RP-related dose values.

Prev | Up | Next
TID 10006 Accumulated Cassette-based Projection Radiography Dose | Home | CT Radiation Dose SR IOD Templates

DICOM PS3.16 2016c - Content Mapping Resource