DICOM PS3.3 2016c - Information Object Definitions

C.8.8.20 Calculated Dose Reference Record Module
Prev | C.8.8 Radiotherapy Modules | Next

#### C.8.8.20 Calculated Dose Reference Record Module

Table C.8-56. Calculated Dose Reference Record Module Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Calculated Dose Reference Sequence | (3008,0070) | 1 | Sequence of doses estimated for each treatment delivery. One or more Items shall be included in this Sequence.
>Referenced Dose Reference Number | (300C,0051) | 1C | Uniquely identifies Dose Reference specified by Dose Reference Number (300A,0012) in Dose Reference Sequence (300A,0010) in RT Prescription Module of referenced RT Plan. Required only if Calculated Dose Reference Number (3008,0072) is not sent. It shall not be present otherwise.
>Calculated Dose Reference Number | (3008,0072) | 1C | Unique identifier of dose reference point within RT Treatment Record IOD. Required only if Referenced Dose Reference Number (300C,0051) is not sent. It shall not be present otherwise.
>Calculated Dose Reference Dose Value | (3008,0076) | 2 | Calculated Dose (Gy).
>Calculated Dose Reference Description | (3008,0074) | 3 | User-defined description of Calculated Dose Reference.

Prev | Up | Next
C.8.8.19 Measured Dose Reference Record Module | Home | C.8.8.21 RT Beams Session Record Module

DICOM PS3.3 2016c - Information Object Definitions