DICOM PS3.4 2016c - Service Class Specifications

CC.2.5.2 Service Class User Behavior
Prev | CC.2.5 Create a Unified Procedure Step (N-CREATE) | Next

#### CC.2.5.2 Service Class User Behavior

An SCU uses N-CREATE to request the SCP schedule a new UPS.

The SCU shall specify in the N-CREATE request primitive the UPS Push SOP Class UID and the SOP Instance UID for the UPS that is to be created and for which Attribute Values are to be provided. See Section CC.3.1 for further discussion of UPS SOP Class UIDs.

The SCU shall provide Attribute values in the N-CREATE request primitive for all required UPS Attributes as specified in Table CC.2.5-3. Additionally, values may be provided for optional Attributes as specified in Table CC.2.5-3.

The SCU shall specify a value of "SCHEDULED" for the Attribute Procedure Step State (0074,1000) in the N-CREATE request primitive.

Prev | Up | Next
CC.2.5 Create a Unified Procedure Step (N-CREATE) | Home | CC.2.5.3 Service Class Provider Behavior

DICOM PS3.4 2016c - Service Class Specifications