DICOM PS3.2 2016c - Conformance

C.4.3.2 Additional Protocols
Prev | C.4.3 Network Interfaces | Next

#### C.4.3.2 Additional Protocols

DHCP support can be configured using the Configuration application. If DHCP is not configured a static IP address is assigned.

If DNS support exists on the local network, then DNS is used for address resolution. The address of the DNS server is retrieved using DHCP if the DHCP option is enabled. If DNS is not supported then the hostnames and addresses are configured in the local hosts file.

Prev | Up | Next
C.4.3 Network Interfaces | Home | C.4.3.3 IPv4 and IPv6 Support

DICOM PS3.2 2016c - Conformance