DICOM PS3.2 2016c - Conformance

G.4.2.2 STORAGE-SCU
Prev | G.4.2 AE Specifications | Next

#### G.4.2.2 STORAGE-SCU

##### G.4.2.2.1 SOP Classes

STORAGE-SCU provides Standard Conformance to the following SOP Class(es) :

Table G.4.2-7. SOP Classes Supported By STORAGE-SCU

SOP Class Name | SOP Class UID | SCU | SCP
--- | --- | --- | ---
Ultrasound Image Storage | 1.2.840.10008.5.1.4.1.1.6.1 | Yes | No
Ultrasound Multi-frame Image Storage | 1.2.840.10008.5.1.4.1.1.3.1 | Yes | No
MR Image Storage | 1.2.840.10008.5.1.4.1.1.4 | Yes | No
Digital Mammography X-Ray Image Storage - For Presentation | 1.2.840.10008.5.1.4.1.1.1.2 | Yes | No
Grayscale Softcopy Presentation State Storage | 1.2.840.10008.5.1.4.1.1.11.1 | Yes | No
Hanging Protocol Storage | 1.2.840.10008.5.1.4.38.1 | Yes | No

Prev | Up | Next
G.4.2 AE Specifications | Home | G.4.2.2.2 Association Policies

DICOM PS3.2 2016c - Conformance