DICOM PS3.3 2016c - Information Object Definitions

F.5.38 Implant Assembly Directory Record Definition
Prev | F.5 Definition of Specific Directory Records | Next

### F.5.38 Implant Assembly Directory Record Definition

The Directory Record is based on the specification of Section F.3. It is identified by a Directory Record Type of Value "IMPLANT ASSY". Table F.5-38 lists the set of keys with their associated Types for such a Directory Record Type. The description of these keys may be found in the Implant Assembly Template IOD. This Directory Record shall be used to reference an Implant Assembly Template SOP Instance.

Table F.5-38. Implant Assembly Keys

Key | Tag | Type | Attribute Description
--- | --- | --- | ---
Implant Assembly Template Name | (0076,0001) | 1 | A name given to the assembly described in this instance.
Manufacturer | (0008,0070) | 1 | Name of the manufacturer that produces the implant.
Procedure Type Code Sequence | (0076,0020) | 1 | A code describing the Intervention in which the implant is used. One or more Items shall be included in this Sequence.
>Include Table 8.8-1 “Code Sequence Macro Attributes” |

### Note

Because (0004,1511) Referenced SOP Instance UID in File may be used as a "pseudo" Directory Record Key (see Table F.3-3), it is not duplicated in this list of keys.

Prev | Up | Next
F.5.37 Implant Directory Record Definition | Home | F.5.39 Implant Group Directory Record Definition

DICOM PS3.3 2016c - Information Object Definitions