DICOM PS3.16 2016c - Content Mapping Resource

CID 6041 Mammography Image Quality Finding
Prev | B DCMR Context Groups (Normative) | Next

## CID 6041 Mammography Image Quality Finding

Type:

  Extensible

Version:

  20020904

Table CID 6041. Mammography Image Quality Finding

Coding Scheme Designator | Code Value | Code Meaning | Source
--- | --- | --- | ---
DCM | 111177 | View and Laterality Marker is missing | MQSA
DCM | 111178 | View and Laterality Marker does not have both view and laterality | MQCM 1999
DCM | 111179 | View and Laterality Marker does not have approved codes | MQCM 1999
DCM | 111180 | View and Laterality Marker is not near the axilla | MQCM 1999
DCM | 111181 | View and Laterality Marker overlaps breast tissue | MQCM 1999
DCM | 111182 | View and Laterality Marker is partially obscured | MQCM 1999
DCM | 111183 | View and Laterality Marker is incorrect |
DCM | 111184 | View and Laterality Marker is off image |
DCM | 111185 | Flash is not near edge of film | MQCM 1999
DCM | 111186 | Flash is illegible, does not fit, or is lopsided | MQSA
DCM | 111187 | Flash doesn't include patient name and additional patient id | MQCM 1999
DCM | 111188 | Flash doesn't include date of examination | MQCM 1999
DCM | 111189 | Flash doesn't include facility name and location | MQSA
DCM | 111190 | Flash doesn't include technologist identification | MQCM 1999
DCM | 111191 | Flash doesn't include cassette/screen/detector identification | MQCM 1999
DCM | 111192 | Flash doesn't include mammography unit identification | MQCM 1999
DCM | 111193 | Date sticker is missing | MQCM 1999
DCM | 111194 | Technical factors missing | MQCM 1999
DCM | 111195 | Collimation too close to breast | MQCM 1999
DCM | 111196 | Inadequate compression | MQCM 1999
DCM | 111197 | MLO Insufficient pectoral muscle | MQCM 1999
DCM | 111198 | MLO No fat is visualized posterior to fibroglandular tissues | MQCM 1999
DCM | 111199 | MLO Poor separation of deep and superficial breast tissues | MQCM 1999
DCM | 111200 | MLO Evidence of motion blur | MQCM 1999
DCM | 111201 | MLO Inframammary fold is not open | MQCM 1999
DCM | 111202 | CC Not all medial tissue visualized | MQCM 1999
DCM | 111203 | CC Nipple not centered on image | MQCM 1999
DCM | 111204 | CC Posterior nipple line does not measure within 1 cm of MLO | MQCM 1999
DCM | 111205 | Nipple not in profile |
DCM | 111206 | Insufficient implant displacement incorrect | MQCM 1999
DCM | 111208 | Grid artifact(s) |
DCM | 111209 | Positioning |
DCM | 111210 | Motion blur |
DCM | 111211 | Under exposed |
DCM | 111212 | Over exposed |
DCM | 111213 | No image |
DCM | 111214 | Detector artifact(s) |
DCM | 111215 | Artifact(s) other than grid or detector artifact |
DCM | 111216 | Mechanical failure |
DCM | 111217 | Electrical failure |
DCM | 111218 | Software failure |
DCM | 111219 | Inappropriate image processing |
DCM | 111220 | Other failure |
DCM | 111221 | Unknown failure |

Prev | Up | Next
CID 6040 Non-lesion Object Type | Home | CID 6042 Status of Results

DICOM PS3.16 2016c - Content Mapping Resource