DICOM PS3.17 2016c - Explanatory Information

JJJ.2 One Single Shot Without Texture Acquisition As Point Cloud
Prev | JJJ Optical Surface Scan | Next

## JJJ.2 One Single Shot Without Texture Acquisition As Point Cloud

Use cases: A single surface record of a patient is made, for example teeth, nose, or breast. If third party software does the post-processing only the point cloud needs to be stored.

The Surface Scan Point Cloud instance will be used because a point cloud is stored. A study with a single series is created.

Figure JJJ.2-1. One Single Shot Without Texture Acquisition As Point Cloud

Prev | Up | Next
JJJ Optical Surface Scan | Home | JJJ.3 One Single Shot With Texture Acquisition As Mesh

DICOM PS3.17 2016c - Explanatory Information